For 1990-2009 cars

## Fan Replacement LLV, LLR

#### Tools Required

• | J 41240-5A Fan Clutch Wrench

• | J 46406 Fan Clutch Remover and Installer

### Removal Procedure

1. Remove the fan shroud. Refer to Engine Coolant Fan Shroud Replacement .
2. Install the J 46406 and the J 41240-5A to the fan clutch.
3. Remove the fan hub nut in a counterclockwise rotation.

### Installation Procedure

Caution: Do not use or attempt to repair a damaged cooling fan assembly. Replace damaged fans with new assemblies. An unbalanced cooling fan could fly apart causing personal injury and property damage.

1. Install the J 46406 and the J 41240-5A to the fan clutch.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the fan hub nut to the pulley and hand tighten in a clockwise rotation.

Tighten
Tighten the fan clutch nut clockwise to 56 N·m (41 lb ft).

3. Install the fan shroud. Refer to Engine Coolant Fan Shroud Replacement .