For 1990-2009 cars

#### Tools Required

J 45951 Front Seal Installer

### Removal Procedure

1. Remove the crankshaft balancer. Refer to Crankshaft Balancer Replacement .

Important: Do not damage the engine front cover or the crankshaft.

2. Pry out the crankshaft front oil seal using a suitable tool and discard the seal.

### Installation Procedure

1. Apply the engine oil to the outside diameter of the crankshaft front oil seal.
2. Use the J 45951 to install the NEW crankshaft front oil seal.
3. Remove the J 45951 .
4. Install the crankshaft balancer. Refer to Crankshaft Balancer Replacement .