For 1990-2009 cars

Connector 1: | X100 Engine Harness to the Front Axle Jumper Harness (4WD)
Connector 2: | X101 Engine Harness to the Fuel Rail Harness (LLV)
Connector 3: | X101 Engine Harness to the Fuel Rail Harness (LLR)
Connector 4: | X102 Body Harness to the Chassis Harness
Connector 5: | X103 Forward Lamp Harness to the Body Harness
Connector 6: | X104 Forward Lamp Harness to the Body Harness
Connector 7: | X105 Engine Harness to the Body Harness (4WD)
Connector 8: | X107 Forward Lamp Harness to Right Front Turn Signal Harness
Connector 9: | X108 Forward Lamp Harness to Left Front Turn Signal Harness
Connector 10: | X109 Engine Harness to Battery Harness (K18)
Connector 11: | X110 Chassis Harness to Engine Harness (UY7)
Connector 12: | X125 Engine Harness to the Body Harness
Connector 13: | X175 Engine Harness to Transmission Harness (M30)
Connector 14: | X200 I/P Harness to the Body Harness
Connector 15: | X201 I/P Harness to the Body Harness
Connector 16: | X202 Driver Door Harness to the Body Harness (AU3)
Connector 17: | X203 I/P Harness to the HVAC Harness
Connector 18: | X204 Steering Column Harness to the I/P Harness
Connector 19: | X208 I/P Harness to the Body Harness
Connector 20: | X209 Body Harness to the Driver Door Harness
Connector 21: | X210 Body Harness to the Passenger Door Harness
Connector 22: | X211 Passenger Door Harness to the Body Harness (AU3)
Connector 23: | X275 SIR Coil Harness to the Body Harness
Connector 24: | X307 Body Harness to the Driver Seat Harness (AG1)
Connector 25: | X310 Dome Lamp Harness to the Body Harness
Connector 26: | X311 Body Harness to the Right Rear Passenger Door Harness (Extended Cab)
Connector 27: | X312 Body Harness to the Left Rear Passenger Door Harness (Extended Cab)
Connector 28: | X313 Body Harness to the Passenger Seat Harness
Connector 29: | X314 Body Harness to the Driver Seat Harness
Connector 30: | X315 Body Harness to the Passenger Seat Harness (AG2)
Connector 31: | X316 Body Harness to the Left Rear Passenger Door Harness (Crew Cab with A31)
Connector 32: | X316 Body Harness to the Left Rear Passenger Door Harness (Crew Cab without A31)
Connector 33: | X316 Body Harness to the Left Rear Passenger Door Harness (Extended Cab)
Connector 34: | X317 Body Harness to the Right Rear Passenger Door Harness (Crew Cab with A31)
Connector 35: | X317 Body Harness to the Right Rear Passenger Door Harness (Crew Cab without A31)
Connector 36: | X317 Body Harness to the Right Rear Passenger Door Harness (Extended Cab)
Connector 37: | X318 Heat Element to Passenger Seat Harness (AG2)
Connector 38: | X319 Heat Element to Driver Seat Harness (AG1)
Connector 39: | X320 Body Harness to Cargo Lamp/Center High Mounted Stop Lamp (CHMSL) Harness
Connector 40: | X400 Chassis Harness to the License Lamp Harness
Connector 41: | X401 Left Rear Lamp Assembly to the Chassis Harness (without Trailer Accessory)
Connector 42: | X401 Trailer Accessory Harness to the Chassis Harness (UY7)
Connector 43: | X402 Right Rear Lamp Assembly to the Chassis Harness
Connector 44: | X403 Left Rear Lamp Assembly to the Trailer Accessory Harness (Trailer Accessory)
Connector 45: | X404 (UY7) Chassis Harness to License Lamp Harness

### X100 Engine Harness to the Front Axle Jumper Harness (4WD)

#### Connector Part Information

- OEM: 15326815
- Service: 15306396
- Description: 4-Way F GT 150 Series Sealed 4.0 (BK)

#### Connector Part Information

- OEM: 15326820
- Service: 15326820
- Description: 4-Way M GT 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X100 Engine Harness to the Front Axle Jumper Harness (4WD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 BK/WH | 1695 | Axle Switch Signal | A | 0.5 BK/WH | 1695 | Axle Switch Signal
B | 0.35 L-BU | 1296 | Axle Actuator - Control | B | 0.35 L-BU | 1296 | Axle Actuator - Control
C | 0.5 PK | 1539 | Ignition Voltage | C | 0.5 PK | 1539 | Ignition Voltage
D | 0.5 BK | 550 | Ground | D | 0.5 BK | 550 | Ground

### X101 Engine Harness to the Fuel Rail Harness (LLV)

#### Connector Part Information

- OEM: 15326822
- Service: 88987186
- Description: 5-Way F GT 150 Series Sealed 4.0 (BK)

#### Connector Part Information

- OEM: 15326827
- Service: 89046648
- Description: 5-Way M GT 150 Series Sealed 4.0 (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X101 Engine Harness to the Fuel Rail Harness (LLV)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 PK | 839 | Ignition Voltage | A | 0.5 PK | 839 | Ignition Voltage
B | 0.5 BK | 1744 | Fuel Injector 1 Control | B | 0.5 BK | 1744 | Fuel Injector 1 Control
C | 0.5 L-GN/BK | 1745 | Fuel Injector 2 Control | C | 0.5 L-GN/BK | 1745 | Fuel Injector 2 Control
D | 0.5 PK/BK | 1746 | Fuel Injector 3 Control | D | 0.5 PK/BK | 1746 | Fuel Injector 3 Control
E | 0.5 L-BU/BK | 844 | Fuel Injector 4 Control | E | 0.5 L-BU/BK | 844 | Fuel Injector 4 Control

### X101 Engine Harness to the Fuel Rail Harness (LLR)

#### Connector Part Information

- OEM: 15326830
- Service: 88953153
- Description: 6-Way F GT 150 Series (BK)

#### Connector Part Information

- OEM: 15326833
- Service: 15326833
- Description: 6-Way M GT 150 Series Sealed 4.0 (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X101 Engine Harness to the Fuel Rail Harness (LLR)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 PK | 839 | Ignition Voltage | A | 0.5 PK | 439 | Ignition Voltage
B | 0.35 L-BU/BK | 844 | Fuel Injector 4 Control | B | 0.5 L-BU/BK | 844 | Fuel Injector 4 Control
C | 0.5 BK/WH | 845 | Fuel Injector 5 Control | C | 0.5 BK/WH | 845 | Fuel Injector 5 Control
D | 0.5 BK | 1744 | Fuel Injector 1 Control | D | 0.5 BK | 1744 | Fuel Injector 1 Control
E | 0.5 L-GN/BK | 1745 | Fuel Injector 2 Control | E | 0.5 L-GN/BK | 1745 | Fuel Injector 2 Control
F | 0.5 PK/BK | 1746 | Fuel Injector 3 Control | F | 0.5 PK/BK | 1746 | Fuel Injector 3 Control

### X102 Body Harness to the Chassis Harness

#### Connector Part Information

- OEM: 15326863
- Service: 15306381
- Description: 16-Way F GT 150 Series, Sealed (BK)

#### Connector Part Information

- OEM: 15326868
- Service: 15306364
- Description: 16-Way M GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See 12191819/8
- Core/Insulation Crimp: Pins: A-F: E/A
- Core/Insulation Crimp: Pins: G-M: 2/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: Pins: A-F: E/4
- Core/Insulation Crimp: Pins: G-M:: E/1
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X102 Body Harness to the Chassis Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 PU | 1589 | Fuel Level Sensor Signal | A | 0.35 PU | 1589 | Fuel Level Sensor Signal
B | 0.35 BK | 2759 | Low Reference | B | 0.35 BK | 2759 | Low Reference
C | 0.35 GY | 2709 | 5-Volt Reference | C | 0.35 GY | 2709 | 5-Volt Reference
D | 0.35 D-GN | 890 | Fuel Tank Pressure Sensor Signal | D | 0.35 D-GN | 890 | Fuel Tank Pressure Sensor Signal
E | 0.35 OG | 1640 | Battery Positive Voltage | E | 0.35 OG | 1640 | Battery Positive Voltage
F | 0.35 WH | 1310 | EVAP Canister Vent Solenoid Control | F | 0.35 WH | 1310 | EVAP Canister Vent Solenoid Control
G | 0.8 BN | 9 | Park Lamp Control | G | 0.8 BN | 9 | Park Lamp Control
H | 1 D-GN | 19 | Right Rear Turn Signal Lamps Control | H | 1 D-GN | 19 | Right Rear Turn Signal Lamps Control
J | 0.8 L-GN | 24 | Backup Lamp Control | J | 0.8 L-GN | 24 | Backup Lamp Control
K | 1 L-BU | 20 | Stop Lamp Control | K | 1 L-BU | 20 | Stop Lamp Control
L | 1 YE | 18 | Left Rear Turn Signal Lamps Control | L | 1 YE | 18 | Left Rear Turn Signal Lamps Control
M | 0.8 BN | 9 | Park Lamp Control | M | 0.8 BN | 9 | Park Lamp Control
N-S | -- | -- | Not Used | N-S | -- | -- | Not Used

### X103 Forward Lamp Harness to the Body Harness

#### Connector Part Information

- OEM: 12052613
- Service: 12085212
- Description: 2-Way F Metri-Pack 480 Series Sealed (BK)

#### Connector Part Information

- OEM: 15336106
- Service: 15306133
- Description: 2-Way M Micro-Pack 480 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12052139/18
- Core/Insulation Crimp: F/3
- Release Tool/Test Probe: 12094430/J-35616-40 (BU)

#### Terminal Part Information

- Terminal/Tray: 12052172/18
- Core/Insulation Crimp: D/3
- Release Tool/Test Probe: 12094430/J-35616-41 (BU)

#### X103 Forward Lamp Harness to the Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 3 RD | 242 | Battery Positive Voltage (UY7) | A | 3 RD | 242 | Battery Positive Voltage
B | 3 RD/WH | 1840 | Battery Positive Voltage (AG1/AG2) | B | 3 RD/WH | 1840 | Battery Positive Voltage (AG1/AG2)

### X104 Forward Lamp Harness to the Body Harness

#### Connector Part Information

- OEM: 15326849
- Service: 88986260
- Description: 12-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15326854
- Service: See Catalog
- Description: 12-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins: A-H, L: E/A
- Core/Insulation Crimp: Pins: J, M: 2/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X104 Forward Lamp Harness to the Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 D-GN | 1409 | Discriminating Sensor - Right - Signal | A | 0.35 D-GN | 1409 | Discriminating Sensor - Right - Signal
B | 0.35 YE | 1834 | Front End Sensor - Voltage | B | 0.35 YE | 1834 | Front End Sensor - Voltage
C | 0.5 D-BU | 15 | Right Turn Signal Lamps Control | C | 0.5 D-BU | 15 | Right Turn Signal Lamps Control
D | 0.35 PU | 544 | DRL Relay Control | D | 0.35 PU | 544 | DRL Relay Control
E | 0.35 YE | 354 | Discriminating Sensor - Signal | E | 0.35 YE | 354 | Discriminating Sensor - Signal
F | 0.35 GY | 349 | Discriminating Sensor - Left - Signal | F | 0.35 GY | 349 | Discriminating Sensor - Left - Signal
G | 0.35 YE | 61 | Low Reference (DF8) | G | 0.35 D-GN | 61 | Low Reference (DF8)
H | 0.35 D-GN/WH | 636 | Ambient Air Temperature Sensor Signal (DF8) | H | 0.35 D-GN/WH | 636 | Ambient Air Temperature Sensor Signal (DF8)
J | 0.8 L-BU | 14 | Left Turn Signal Lamp Control | J | 0.8 L-BU | 14 | Left Turn Signal Lamp Control
K | -- | -- | Not Used | K | -- | -- | Not Used
L | 0.5 TN | 848 | Brake Switch Signal | L | -- | -- | Not Used
M | 0.8 L-BU | 20 | Stop Lamp Control | M | -- | -- | Not Used

### X105 Engine Harness to the Body Harness (4WD)

#### Connector Part Information

- OEM: 15326842
- Service: 15326843
- Description: 10-Way F GT150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15326847
- Service: 19151490
- Description: 10-Way M GT150 Series Sealed 4.0 (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X105 Engine Harness to the Body Harness (4WD)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 BK | 1552 | Motor Control A | A | 0.5 BK | 1552 | Motor Control A
B | 0.5 RD | 1553 | Motor Control B | B | 0.5 RD | 1553 | Motor Control B
C | 0.35 TN | 1569 | 2WD/4WD Signal | C | 0.35 TN | 1569 | 2WD/4WD Signal
D | 0.35 RD/WH | 1556 | Channel C Encoder - Signal | D | 0.35 RD/WH | 1556 | Channel C Encoder - Signal
E | 0.35 GY | 2281 | Neutral Switch Signal | E | 0.35 GY | 2281 | Neutral Switch Signal
F | 0.35 YE/BK | 1558 | Channel B Encoder - Signal | F | 0.35 YE/BK | 1558 | Channel B Encoder - Signal
G | 0.5 BK/WH | 1695 | Axle Switch Signal | G | 0.35 BK/WH | 1695 | Axle Switch Signal
H | 0.35 L-BU | 1296 | Axle Actuator - Control | H | 0.35 L-BU | 1296 | Axle Actuator - Control
J | 0.35 D-BU/WH | 1557 | Channel A Encoder - Signal | J | 0.35 D-BU/WH | 1557 | Channel A Encoder - Signal
K | 0.35 BN/WH | 1555 | Channel P Encoder - Signal | K | 0.35 BN/WH | 1555 | Channel P Encoder - Signal

### X107 Forward Lamp Harness to Right Front Turn Signal Harness

#### Connector Part Information

- OEM: 12110293
- Service: 12117025
- Description: 3-Way F Metri-Pack 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 12129615
- Service: 15305889
- Description: 3-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X107 Forward Lamp Harness to Right Front Turn Signal Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 BN | 9 | Park Lamp Control | A | BN | -- | Park Lamp Control
B | 0.5 D-BU | 15 | Right Turn Signal Lamps Control | B | L-BU | -- | Right Turn Signal Lamps Control
C | 0.5 BK | 850 | Ground | C | BK | -- | Ground

### X108 Forward Lamp Harness to Left Front Turn Signal Harness

#### Connector Part Information

- OEM: 12110293
- Service: 12117025
- Description: 3-Way F Metri-Pack 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 12129615
- Service: 15305889
- Description: 3-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X108 Forward Lamp Harness to Left Front Turn Signal Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 BN | 9 | Park Lamp Control | A | BN | -- | Park Lamp Control
B | 0.5 L-BU | 14 | Left Turn Signal Supply Lamps Voltage | B | L-BU | -- | Left Turn Signal Supply Lamps Voltage
C | 0.5 BK | 850 | Ground | C | BK | -- | Ground

### X109 Engine Harness to Battery Harness (K18)

#### Connector Part Information

- OEM: 15326120
- Service: See Catalog
- Description: 1-Way F Maxi Sealed (BK)

#### Connector Part Information

- OEM: 15326119
- Service: See Catalog
- Description: 1-Way M Maxi Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15336748/20
- Core/Insulation Crimp: F/3
- Release Tool/Test Probe: 12150860/J-35616-44 (YE)

#### Terminal Part Information

- Terminal/Tray: Not Serviceable in Kit
- Core/Insulation Crimp: Not Serviceable in Kit
- Release Tool/Test Probe: Not Serviceable in Kit

#### X109 Engine Harness to Battery Harness (K18)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 5 RD | 1 | Battery Positive Voltage | 1 | 8 RD | 1 | Battery Positive Voltage

### X110 Chassis Harness to Engine Harness (UY7)

#### Connector Part Information

- OEM: 12146314
- Service: See Catalog
- Description: 1-Way F Metri-Pack 280 Series Sealed (BK)

#### Connector Part Information

- OEM: 12065172
- Service: See Catalog
- Description: 1-Way M Metri-Pack 280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12077413/4
- Core/Insulation Crimp:F/5
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: 12129497/1
- Core/Insulation Crimp:F/5
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### X110 Chassis Harness to Engine Harness (UY7)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 3 RD | 742 | Battery Positive Voltage | A | 3 RD/BK | 742 | Battery Positive Voltage

### X125 Engine Harness to the Body Harness

#### Connector Part Information

- OEM: 15326856
- Service: 88986261
- Description: 14-Way F 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15326861
- Service: 88986246
- Description: 14-Way M 150 Series Sealed 4.0 (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X125 Engine Harness to the Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.8 PU | 421 | AIR Solenoid Control (K18) | A | 0.8 PU | 421 | AIR Solenoid Control (K18)
B | 0.35 PU | 1807 | Class 2 Serial Data | B | 0.35 PU | 1807 | Class 2 Serial Data
C | 0.5 TN/WH | 2500 | High Speed GMLAN Serial Data (-) | C | 0.5 TN/WH | 2500 | High Speed GMLAN Serial Data (-)
D | 0.5 TN | 2501 | High Speed GMLAN Serial Data (+) | D | 0.5 TN | 2501 | High Speed GMLAN Serial Data (+)
E | 0.5 BN | 4 | Ignition Voltage (M30) | E | 0.5 BN | 4 | Ignition Voltage (M30)
F | 0.35 L-BU | 20 | Stop Lamp Control | F | 0.8 L-BU | 20 | Stop Lamp Control (M30)
G | 0.5 PK | 739 | Ignition Voltage | G | 0.5 PK | 739 | Ignition Voltage
H | 0.35 OG/BK | 463 | Requested Torque Signal (2WD) | H | 0.35 OG/BK | 463 | Requested Torque Signal (2WD)
J | 0.35 TN/BK | 464 | Delivered Torque Signal (2WD) | J | 0.35 TN/BK | 464 | Delivered Torque Signal (2WD)
K | 0.5 D-GN/WH | 6294 | Low Reference (MA5) | K | 0.35 D-GN/WH | 6294 | Low Reference
L | 0.5 D-GN | 6293 | 5-Volt Reference (MA5) | L | 0.35 D-GN | 6293 | 5-Volt Reference
M | 0.5 D-BU | 6306 | Clutch Pedal Position Sensor Signal (MA5) | M | 0.35 D-BU | 6306 | Clutch Pedal Position Sensor Signal
N | 0.35 BN | 441 | Ignition Voltage | N | -- | -- | Not Used
P | -- | -- | Not Used | P | -- | -- | Not Used

### X175 Engine Harness to Transmission Harness (M30)

#### Connector Part Information

- OEM: 13524840
- Service: See Catalog
- Description: 20-Way F Micro-Pack 100 W Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12084913
- Core/Insulation Crimp: W/W
- Release Tool/Test Probe: 12122523/J-35616-6 (BN)

#### Connector Part Information

- OEM: 15443076
- Service: See Catalog
- Description: 20-Way M Micro-Pack 100 W Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12160551/3
- Core/Insulation Crimp: W/W
- Release Tool/Test Probe: 12122523/J-35616-7 (BN)

#### X175 Engine Harness to Transmission Harness (M30)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 L-GN | 1222 | 1-2 Shift Solenoid Valve Control | A | 0.5 L-GN | 1222 | 1-2 Shift Solenoid Valve Control
B | 0.5 YE/BK | 1223 | 2-3 Shift Solenoid Valve Control | B | 0.5 YE | 1223 | 2-3 Shift Solenoid Valve Control
C | 0.5 RD/BK | 1228 | PC Solenoid Valve High Control | C | 0.5 PU | 1228 | PC Solenoid Valve High Control
D | 0.5 L-BU/WH | 1229 | PC Solenoid Valve Low Control | D | 0.5 L-BU | 1229 | PC Solenoid Valve Low Control
E | 0.5 PK | 139 | Ignition Voltage | E | 0.5 RD | 839 | Ignition Voltage
F-J | -- | -- | Not Available | F-J | -- | -- | Not Used
K | 0.35 BN/WH | 6254 | ISS Signal | K | 0.5 BK | 1230 | ISS Signal
L | 0.5 YE/BK | 1227 | TFT Sensor Signal | L | 0.5 BN | 1227 | TFT Sensor Signal
M | 0.5 BK | 452 | Low Reference | M | 0.5 GY | 452 | Low Reference
N | 0.5 PK | 1224 | Transmission Fluid Pressure Switch Signal A | N | 0.5 PK | 1224 | Transmission Fluid Pressure Switch Signal A
P | 0.5 RD | 1226 | Transmission Fluid Pressure Switch Signal C | P | 0.5 OG | 1226 | Transmission Fluid Pressure Switch Signal C
R | 0.5 D-BU | 1225 | Transmission Fluid Pressure Switch Signal B | R | 0.5 D-BU | 1225 | Transmission Fluid Pressure Switch Signal B
S | 0.5 WH | 687 | 3-2 Shift Solenoid Valve Control | S | 0.5 WH | 687 | 3-2 Shift Solenoid Valve Control
T | 0.5 TN/BK | 422 | TCC Solenoid Valve Control | T | 0.5 BK | 422 | TCC Solenoid Valve Control
U | 0.5 BN | 418 | TCC PWM Solenoid Valve Control | U | 0.5 TN | 418 | TCC PWM Solenoid Valve Control
V | 0.35 D-BU | 6253 | Low Reference | V | 0.5 D-GN | 1231 | Low Reference
W | -- | -- | Not Available | W | -- | -- | Not Used

### X200 I/P Harness to the Body Harness

#### Connector Part Information

- OEM: 15304837
- Service: 15359287
- Description: 40-Way F GT 150, 280 Series (BK)

#### Connector Part Information

- OEM: 15359284
- Service: 88988307
- Description: 40-Way M GT 150, 280 Series (BK)

#### Terminal Part Information

- Pins: A2-A6, A8, B1, B4-B6, B8-B9, B12, C1-C2, C7, C9-C10, C12, D1, D4-D6, D8
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: A2-A3, A5-A6, A8, B1, B4-B5, B6, B8-B9, B12, C1-C2, C7, C9-C10, C12, D1, D4-D6, D8
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X200 I/P Harness to the Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | -- | -- | Not Used | A1 | -- | -- | Not Used
A2 | 0.35 D-GN | 2308 | Passenger Airbag On Indicator Control | A2 | 0.35 D-GN | 2308 | Passenger Airbag On Indicator Control
A3 | 0.35 L-BU/BK | 1693 | Switch Signal Low (4WD) | A3 | 0.35 L-BU | 1693 | Switch Signal Low (4WD)
A4 | 2 BK/WH | 1151 | Ground | A4 | 2 BK/WH | 1151 | Not Used
A5 | 0.8 OG | 40 | Battery Positive Voltage | A5 | 0.8 OG | 40 | Battery Positive Voltage
OG | 0.8 40 | Battery Positive Voltage
A6 | 0.35 PK | 339 | Ignition Voltage | A6 | 0.35 PK | 339 | Ignition Voltage
0.35 PK | 339 | Ignition Voltage (4WD)
A7 | -- | -- | Not Used | A7 | -- | -- | Not Used
A8 | 0.35 BN | 141 | Ignition Voltage | A8 | 0.35 BN | 141 | Ignition Voltage
B1 | 0.5 OG | 1440 | Battery Positive Voltage | B1 | 0.5 OG | 1440 | Battery Positive Voltage
B2-B3 | -- | -- | Not Used | B2-B3 | -- | -- | Not Used
B4 | 0.35 GY | 91 | Windshield Wiper Relay Control | B4 | 0.35 GY | 91 | Windshield Wiper Relay Control
B5 | 0.35 GY/BK | 1694 | 5-Volt Reference (4WD) | B5 | 0.35 GY/BK | 1694 | 5-Volt Reference (4WD)
B6 | 0.35 GY | 1884 | Cruise Control Set/Coast and Resume/Accelerate Switch Signal (K34) | B6 | 0.35 GY | 1884 | Cruise Control Set/Coast and Resume/Accelerate Switch Signal (K34)
B7 | -- | -- | Not Used | B7 | -- | -- | Not Used
B8 | 0.35 BN | 1560 | Neutral Indicator Control (4WD) | B8 | 0.35 BN | 1560 | Neutral Indicator Control (4WD)
B9 | 0.35 L-GN/BK | 1563 | 2 HI Indicator - Control (4WD) | B9 | 0.35 L-GN/BK | 1563 | 2 HI Indicator - Control (4WD)
B10-B11 | -- | -- | Not Used | B10-B11 | -- | -- | Not Used
B12 | 0.5 YE | 116 | Left Rear Speaker Output (-) (Extended/Crew Cab) | B12 | 0.5 YE | 116 | Left Rear Speaker Output (-) (Extended/Crew Cab)
C1 | 0.5 BN | 199 | Left Rear Speaker Output (+) (Extended/Crew Cab) | C1 | 0.5 BN | 199 | Left Rear Speaker Output (+) (Extended/Crew Cab)
C2 | 0.5 OG | 1740 | Battery Positive Voltage | C2 | 0.5 OG | 1740 | Battery Positive Voltage
C3-C6 | -- | -- | Not Used | C3-C6 | -- | -- | Not Used
C7 | 0.35 PU/WH | 1565 | 4 LO Indicator - Control (4WD) | C7 | 0.35 PU/WH | 1565 | 4 LO Indicator - Control (4WD)
C8 | -- | -- | Not Used | C8 | -- | -- | Not Used
C9 | 0.35 BN | 9 | Park Lamp Control | C9 | 0.35 BN | 9 | Park Lamp Control
C10 | 0.35 TN/BK | 1566 | 4 HI Indicator - Control (4WD) | C10 | 0.35 TN/BK | 1566 | 4 HI Indicator - Control (4WD)
C11 | -- | -- | Not Used | C11 | -- | -- | Not Used
C12 | 0.35 D-BU | 2307 | Passenger Airbag On Indicator Control | C12 | 0.35 D-BU | 2307 | Passenger Airbag On Indicator Control
D1 | 0.8 OG | 240 | Battery Positive Voltage (KC5) | D1 | 0.8 OG | 240 | Battery Positive Voltage (KC5)
D2-D3 | -- | -- | Not Used | D2-D3 | -- | -- | Not Used
D4 | 0.5 GY | 118 | Left Front Speaker Output (-) | D4 | 0.5 GY | 118 | Left Front Speaker Output (-)
D4 | 0.5 GY | 118 | Left Front Speaker Output (-) (UQ3)
D5 | 0.5 TN | 201 | Left Front Speaker Output (+) | D5 | 0.5 TN | 201 | Left Front Speaker Output (+)
0.5 TN | 201 | Left Front Speaker Output (+) (UQ3)
D6 | 1 OG | 1140 | Battery Positive Voltage | D6 | 1 OG | 1140 | Battery Positive Voltage
0.5 OG | 1140 | Battery Positive Voltage (U2K)
D7 | -- | -- | Not Used | D7 | -- | -- | Not Used
D8 | 0.5 YE | 143 | Ignition Voltage | D8 | 0.5 YE | 143 | Ignition Voltage

### X201 I/P Harness to the Body Harness

#### Connector Part Information

- OEM: 15317325
- Service: 15317325
- Description: 22-Way F GT 150, 280 Series (L-GY)

#### Connector Part Information

- OEM: 15317322
- Service: 15317322
- Description: 22-Way M GT 150, 280 Series (L-GY)

#### Terminal Part Information

- Pins: A1-A3, A9-A11, B9-B11
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: A7, B4-B5, B7-B8
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: Pins: A7: 2/A
- Core/Insulation Crimp: Pins: B4-B5, B7-B8: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: A4-A5, A8
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: 4/4
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Pins: A1-A3, A9-A11, B9-B11
- Terminal/Tray: 15304702/19
- Core/Insulation Crimp: Pins: A1-A3, A9, B9: E/C
- Core/Insulation Crimp: Pins: A10-A11, B10-B11: E/4
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: B4-B5
- Terminal/Tray: 15304722/8
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

- Pins: A4-A5, A7-A8, B7-B8
- Terminal/Tray: 15304724/8
- Core/Insulation Crimp: Pins: A4-A5, A8: C/D
- Core/Insulation Crimp: Pins: A7: 2/A
- Core/Insulation Crimp: Pins: B7-B8: See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### X201 I/P Harness to the Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | 0.35 BN/WH | 419 | MIL Control | A1 | 0.35 BN/WH | 419 | MIL Control
A2 | 0.35 D-GN/WH | 2514 | Keypad Signal (UE1) | A2 | 0.35 D-GN/WH | 2514 | Keypad Signal (UE1)
A3 | 0.35 L-GN/BK | 2515 | Keypad Control (UE1) | A3 | 0.35 L-GN/BK | 2515 | Keypad Control (UE1)
A4 | 2 BK | 2050 | Ground | A4 | 2 BK | 2050 | Ground
A5 | 2 BK | 2050 | Ground | A5 | 2 BK | 2050 | Ground
A6 | -- | -- | Not Used | A6 | -- | -- | Not Used
A7 | 0.8 OG | 340 | Battery Positive Voltage (UE1) | A7 | 0.8 OG | 340 | Battery Positive Voltage (UE1)
A8 | 2 BN | 41 | Ignition Voltage | A8 | 2 BN | 41 | Ignition Voltage
A9 | 0.35 D-GN/WH | 762 | A/C Request Signal (C60) | A9 | 0.35 D-GN/WH | 762 | A/C Request Signal (C60)
A10 | 0.5 GY | 655 | Cellular Microphone Signal (UE1) | A10 | 0.5 GY | 655 | Cellular Microphone Signal (UE1)
A11 | 0.5 BARE | 1705 | Drain Wire (UE1) | A11 | 0.5 BARE | 1705 | Drain Wire (UE1)
B1-B3 | -- | -- | Not Used | B1-B3 | -- | -- | Not Used
B4 | 0.35 YE/BK | 2516 | Keypad Green LED Signal (UE1) | B4 | 0.35 YE/BK | 2516 | Keypad Green LED Signal (UE1)
B5 | 0.35 BN/WH | 2517 | Keypad Red LED Signal (UE1) | B5 | 0.35 BN/WH | 2517 | Keypad Red LED Signal (UE1)
B6 | -- | -- | Not Used | B6 | -- | -- | Not Used
B7 | 0.5 D-GN | 117 | Right Front Speaker Output (-) | B7 | 0.5 D-GN | 117 | Right Front Speaker Output (-)
0.5 D-GN | 117 | Right Front Speaker Output (-)
B8 | 0.5 L-GN | 200 | Right Front Speaker Output (+) | B8 | 0.5 L-GN | 200 | Right Front Speaker Output (+)
0.5 L-GN | 200 | Right Front Speaker Output (+) (UQ3)
B9 | -- | -- | Not Used | B9 | -- | -- | Not Used
B10 | 0.5 D-BU | 46 | Right Rear Speaker Output (+) | B10 | 0.5 D-BU | 46 | Right Rear Speaker Output (+)
B11 | 0.5 L-BU | 115 | Right Rear Speaker Output (-) | B11 | 0.5 L-BU | 115 | Right Rear Speaker Output (-)

### X202 Driver Door Harness to the Body Harness (AU3)

#### Connector Part Information

- OEM: 15410450
- Service: 89047131
- Description: 9-Way F Ducon 1.5 (WH)

#### Connector Part Information

- OEM: 12185085
- Service: 88953417
- Description: 9-Way M Ducon 1.5 (WH)

#### Terminal Part Information

- Pins: 1-4, 6-9
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: 1-4, 6-9
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X202 Driver Door Harness to the Body Harness (AU3)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 BN | 9 | Park Lamp Control | 1 | 0.5 BN | 9 | Park Lamp Control
0.5 BN | 9 | Park Lamp Control
2 | 2 YE | 443 | Ignition Voltage | 2 | 2 YE | 443 | Ignition Voltage
3 | 0.8 GY | 295 | Door Lock Actuator Lock Control | 3 | 0.8 GY | 295 | Door Lock Actuator Lock Control
0.8 GY | 295 | Door Lock Actuator Lock Control
4 | 1 BK | 850 | Ground (ZQ6) | 4 | 1 BK | 850 | Ground (ZQ6)
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | 0.35 L-BU | 244 | Passenger Door Lock Switch Lock Control | 6 | 0.35 L-BU | 244 | Passenger Door Lock Switch Lock
0.35 L-BU | 244 | Passenger Door Lock Switch Lock
7 | 0.35 WH | 194 | Door Unlock Control | 7 | 0.35 WH | 194 | Door Unlock Control
8 | 0.8 OG | 1240 | Battery Positive Voltage | 8 | 0.8 OG | 1240 | Battery Positive Voltage
9 | 0.8 TN | 294 | Door Lock Actuator Unlock Control | 9 | 0.8 TN | 294 | Door Lock Actuator Unlock Control

### X203 I/P Harness to the HVAC Harness

#### Connector Part Information

- OEM: 15326931
- Service: 15306309
- Description: 10-Way F GT 280 Series (BK)

#### Connector Part Information

- OEM: 15326935
- Service: 15306305
- Description: 10-Way M GT 280 Series (BK)

#### Terminal Part Information

- Pins: A, C, E, G, J
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: 4/4
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: B, D, F, H, K
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Pins: A, C, E, G, J
- Terminal/Tray: 15304724/8
- Core/Insulation Crimp: A/D
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

- Pins: B, D, F, H, K
- Terminal/Tray: 15304722/8
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### X203 I/P Harness to the HVAC Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 2 YE | 60 | Blower Motor Low Control | A | 2 YE | 60 | Blower Motor Low Control
B | 0.35 L-GN/BK | 1647 | Recirculation Door Control B | B | 0.35 L-GN/BK | 1647 | Recirculation Door Control B (C60)
C | 2 TN | 63 | Blower Motor Medium 1 Control | C | 2 TN | 63 | Blower Motor Medium 1 Control
D | 0.35 PK/WH | 1648 | Recirculation Door Control A | D | 0.35 PK/WH | 1648 | Recirculation Door Control A (C60)
E | 2 L-BU | 72 | Medium 2 Blower Motor Control | E | 2 L-BU | 72 | Medium 2 Blower Motor Control
F | 0.35 L-GN | 66 | A/C Request Signal | F | 0.35 L-GN | 66 | A/C Request Signal (C60)
G | 2 OG | 52 | Blower Motor High Control | G | 2 OG | 52 | Blower Motor High Control
H | 0.35 D-GN/WH | 762 | A/C Request Signal | H | 0.35 D-GN/WH | 762 | A/C Request Signal (C60)
J | 2 BN | 41 | Ignition Voltage | J | 2 BN | 41 | Ignition Voltage
K | 0.35 BK | 2050 | Ground | K | 0.35 BK | 2050 | Ground (C60)

### X204 Steering Column Harness to the I/P Harness

#### Connector Part Information

- OEM: 15317325
- Service: 15317325
- Description: 22-Way F GT 150, 280 Series (L-GY)

#### Connector Part Information

- OEM: 15317322
- Service: 15317322
- Description: 22-Way M GT 150, 280 Series (L-GY)

#### Terminal Part Information

- Pins: A1-A8, B1, B3-B5, B7-B11, A10, A11
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: A1-A3, B1, B3, B9-B11, A10-A11
- Terminal/Tray: 15304702/19
- Core/Insulation Crimp: Pins: A1-A3, B3: E/4
- Core/Insulation Crimp: Pins: B1, B9-B11, A10-A11: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: A4-A7, B4-B5, B7-B8
- Terminal/Tray: 15304722/8
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

- Pins: A8
- Terminal/Tray: 15304724/8
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### X204 Steering Column Harness to the I/P Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | 0.5 WH/BU | 1390 | Ignition Voltage | A1 | 0.5 WH | 1390 | Ignition Voltage
A2 | 0.5 WH/GN | 338 | Ignition Voltage | A2 | 0.5 D-BU | 338 | Ignition Voltage
A3 | 0.5 WH/RD | 4 | Ignition Voltage | A3 | 0.5 BN | 4 | Ignition Voltage
A4 | 0.35 GY | 323 | Shift Solenoid Control | A4 | 0.35 BN | 323 | Shift Solenoid Control
A5 | 0.5 BN | 228 | Windshield Washer Pump Control | A5 | 0.5 RD | 228 | Windshield Washer Pump Control
A6 | 0.35 D-BU/BK | 91 | Windshield Wiper Relay Control | A6 | 0.35 GY | 91 | Windshield Wiper Relay Control
A7 | 0.35 D-BU/RD | 112 | Windshield Wiper Switch Signal 1 | A7 | 0.35 GY | 112 | Windshield Wiper Switch Signal 1
A8 | 0.35 YE | 339 | Ignition Voltage | A8 | 0.35 PK | 339 | Ignition Voltage
0.35 PK | 339 | Ignition Voltage
A9 | -- | -- | Not Used | A9 | -- | -- | Not Used
A10 | 0.35 D-BU/WH | 1356 | Flash-To-Pass Switch Signal | A10 | 0.35 BN | 1356 | Flash-To-Pass Switch Signal
A11 | 0.35 RD | 524 | Headlamp Dimmer Switch High Beam Signal | A11 | 0.35 PU | 524 | Headlamp Dimmer Switch High Beam Signal
B1 | 0.35 WH/YE | 1073 | Ignition Key Resistor Signal | B1 | 0.35 WH/BK | 1073 | Ignition Key Resistor Signal
B2 | -- | -- | Not Used | B2 | -- | -- | Not Used
B3 | 0.5 WH/BK | 1740 | Battery Positive Voltage | B3 | 0.5 OG | 1740 | Battery Positive Voltage
B4 | 0.35 D-BU | 2050 | Ground | B4 | 0.35 BK | 2050 | Ground
B5 | 0.35 PU | 1508 | Turn Signal Switch Signal | B5 | 0.35 L-BU | 1508 | Turn Signal Switch Signal
B6 | -- | -- | Not Used | B6 | -- | -- | Not Used
B7 | 0.5 BK | 143 | Ignition Voltage | B7 | 0.5 YE | 143 | Ignition Voltage
B8 | 0.35 WH | 1884 | Cruise Control Set/Coast and Resume/Accelerate Switch Signal | B8 | 0.35 GY | 1884 | Cruise Control Set/Coast and Resume/Accelerate Switch Signal
B9 | 0.35 D-GN | 2050 | Ground | B9 | 0.35 BK | 2050 | Ground
B10 | 0.35 PK | 2050 | Ground | B10 | 0.35 BK | 2050 | Ground
B11 | 0.35 L-GN | 28 | Horn Relay Control | B11 | 0.35 BK | 28 | Horn Relay Control

### X208 I/P Harness to the Body Harness

#### Connector Part Information

- OEM: 15424638
- Service: 88987926
- Description: 4-Way F Metri-Pack 280 Series (YE)

#### Connector Part Information

- OEM: 15424636
- Service: 88987842
- Description: 4-Way M Metri-Pack 280 Series (YE)

#### Terminal Part Information

- Pins: A1-A2, B1-B2
- Terminal/Tray: 12034046/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Terminal Part Information

- Pins: A1-A2, B1-B2
- Terminal/Tray: 12034047/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### X208 I/P Harness to the Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | 0.5 OG | 3024 | I/P Module - Stage 1 - Low Control | A1 | 0.5 OG | 3024 | I/P Module - Stage 1 - Low Control
A2 | 0.5 YE | 3025 | I/P Module - Stage 1 - High Control | A2 | 0.5 YE | 3025 | I/P Module - Stage 1 - High Control
B1 | 0.5 GY | 3027 | I/P Module - Stage 2 - High Control | B1 | 0.5 GY | 3027 | I/P Module - Stage 2 - High Control
B2 | 0.5 PU | 3026 | I/P Module - Stage 2 - Low Control | B2 | 0.5 PU | 3026 | I/P Module - Stage 2 - Low Control

### X209 Body Harness to the Driver Door Harness

#### Connector Part Information

- OEM: 15427364
- Service: 88953422
- Description: 18-Way F 040 III (WH)

#### Connector Part Information

- OEM: 15427361
- Service: 88953391
- Description: 18-Way M 040 III (WH)

#### Terminal Part Information

- Pins: 1-18
- Terminal/Tray: 15445905/23
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12180559/J-35616-6 (BN)

#### Terminal Part Information

- Pins: 1-18
- Terminal/Tray: 15355486/20
- Core/Insulation Crimp: C/E/C
- Release Tool/Test Probe: 15315247/J-35616-13 (BU)

#### X209 Body Harness to the Driver Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 RD/WH | 881 | Passenger Mirror Motor Right Control (A31) | 1 | 0.35 RD/WH | 881 | Passenger Mirror Motor Right Control (A31)
2 | 0.35 D-BU | 1307 | Power Window Master Switch Lockout Signal (A31) | 2 | 0.35 D-BU | 1307 | Power Window Master Switch Lockout Signal (A31)
3 | 0.35 BN/WH | 1498 | Passenger Mirror Motor Up Control (DE6) | 3 | 0.35 BN/WH | 1498 | Passenger Mirror Motor Up Control (DE6)
4 | 0.5 TN | 201 | Left Front Speaker Output (+) (UQ3) | 4 | 0.5 TN | 201 | Left Front Speaker Output (+) (UQ3)
5 | 0.5 GY | 118 | Left Front Speaker Output (-) (UQ3) | 5 | 0.5 GY | 118 | Left Front Speaker Output (-) (UQ3)
6 | 0.35 TN | 167 | Power Window Master Switch Right Front Down Signal (A31) | 6 | 0.35 TN | 167 | Power Window Master Switch Right Front Down Signal (A31)
7 | 0.35 D-GN | 168 | Power Window Master Switch Left Rear Up Signal (Crew Cab) (A31) | 7 | 0.35 D-GN | 168 | Power Window Master Switch Left Rear Up Signal (Crew Cab) (A31)
8 | 0.35 L-BU | 166 | Power Window Master Switch Right Front Up Signal (A31) | 8 | 0.35 L-BU | 166 | Power Window Master Switch Right Front Up Signal (A31)
9 | 0.35 L-GN | 170 | Power Window Master Switch Right Rear Up Signal (A31) | 9 | 0.35 L-GN | 170 | Power Window Master Switch Right Rear Up Signal (Crew Cab) (A31)
10 | 0.35 YE | 1187 | Power Window Master Switch Left Rear Down Signal (Crew Cab) (A31) | 10 | 0.35 YE | 1187 | Power Window Master Switch Left Rear Down Signal (Crew Cab) (A31)
11 | 0.5 TN | 201 | Left Front Speaker Output (+) | 11 | 0.5 TN | 201 | Left Front Speaker Output (+)
12 | 0.5 GY | 118 | Left Front Speaker Output (-) | 12 | 0.5 GY | 118 | Left Front Speaker Output (-)
13 | 0.35 YE | 2131 | Side Impact Sensing Module - Left -Voltage (ASF) | 13 | 0.35 YE | 2131 | Side Impact Sensing Module - Left -Voltage (ASF)
14 | 0.35 WH | 2132 | Side Impact Sensing Module - Left - Signal (ASF) | 14 | 0.35 WH | 2132 | Side Impact Sensing Module - Left - Signal (ASF)
15 | 0.35 OG | 1732 | Courtesy Lamps Control | 15 | 0.35 OG | 1732 | Courtesy Lamps Control
16 | 0.35 D-BU | 245 | Passenger Door Lock Switch Unlock Control (A31) | 16 | 0.35 D-BU | 245 | Passenger Door Lock Switch Unlock Control (A31)
17 | 0.35 L-BU/WH | 1497 | Passenger Mirror Motor Left/Down Control (DE6) | 17 | 0.35 L-BU/WH | 1497 | Passenger Mirror Motor Left/Down Control (DE6)
18 | 0.35 PU | 171 | Power Window Master Switch Right Rear Down Signal (Crew Cab) (A31) | 18 | 0.35 PU | 171 | Power Window Master Switch Right Rear Down Signal (Crew Cab) (A31)

### X210 Body Harness to the Passenger Door Harness

#### Connector Part Information

- OEM: 15427364
- Service: 88953422
- Description: 18-Way F 040 III (WH)

#### Connector Part Information

- OEM: 15427361
- Service: 88953391
- Description: 18-Way M 040 III (WH)

#### Terminal Part Information

- Pins: 1-18
- Terminal/Tray: 15445905/23
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12180559/J-35616-6 (BN)

#### Terminal Part Information

- Pins: 1-18
- Terminal/Tray: 15355486/20
- Core/Insulation Crimp: C/E/C
- Release Tool/Test Probe: 15315247/J-35616-13 (BU)

#### X210 Body Harness to the Passenger Door Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 RD/WH | 881 | Passenger Mirror Motor Right Control (DE6) | 1 | 0.35 RD/WH | 881 | Passenger Mirror Motor Right Control (DE6)
2 | 0.35 D-BU | 1307 | Power Window Master Switch Lockout Signal (A31) | 2 | 0.35 D-BU | 1307 | Power Window Master Switch Lockout Signal (A31)
3 | 0.35 BN/WH | 1498 | Passenger Mirror Motor Up Control (DE6) | 3 | 0.35 BN/WH | 1498 | Passenger Mirror Motor Up Control (DE6)
4 | 0.5 L-GN | 200 | Right Front Speaker Output (+) | 4 | 0.5 L-GN | 200 | Right Front Speaker Output (+) (UQ3)
5 | 0.5 D-GN | 117 | Right Front Speaker Output (-) | 5 | 0.5 D-GN | 117 | Right Front Speaker Output (-) (UQ3)
6 | 0.35 TN | 167 | Power Window Master Switch Right Front Down Signal (A31) | 6 | 0.35 TN | 167 | Power Window Master Switch Right Front Down Signal (A31)
7 | 0.35 BN | 9 | Park Lamp Control (A31) | 7 | 0.35 BN | 9 | Park Lamp Control (A31)
8 | 0.35 L-BU | 166 | Power Window Master Switch Right Front Up Signal (A31) | 8 | 0.35 L-BU | 166 | Power Window Master Switch Right Front Up Signal (A31)
9 | -- | -- | Not Used | 9 | -- | -- | Not Used
10 | 0.35 L-BU | 244 | Passenger Door Lock Switch Lock Control (A31) | 10 | 0.35 L-BU | 244 | Passenger Door Lock Switch Lock Control (A31)
11 | 0.5 L-GN | 200 | Right Front Speaker Output (+) | 11 | 0.5 L-GN | 200 | Right Front Speaker Output (+)
12 | 0.5 D-GN | 117 | Right Front Speaker Output (-) | 12 | 0.5 D-GN | 117 | Right Front Speaker Output (-)
13 | 0.35 TN | 2133 | Side Impact Sensing Module - Right - Voltage (ASF) | 13 | 0.35 TN | 2133 | Side Impact Sensing Module - Right - Voltage (ASF)
14 | 0.35 D-GN | 2134 | Side Impact Sensing Module - Right - Signal (ASF) | 14 | 0.35 D-GN | 2134 | Side Impact Sensing Module - Right - Signal (ASF)
15 | -- | -- | Not Used | 15 | -- | -- | Not Used
16 | 0.35 D-BU | 245 | Passenger Door Lock Switch Unlock Control (A31) | 16 | 0.35 D-BU | 245 | Passenger Door Lock Switch Unlock Control (A31)
17 | 0.35 L-BU/WH | 1497 | Passenger Mirror Motor Left/Down Control (A31) | 17 | 0.35 L-BU/WH | 1497 | Passenger Mirror Motor Left/Down Control (A31)
18 | -- | -- | Not Used | 18 | -- | -- | Not Used

### X211 Passenger Door Harness to the Body Harness (AU3)

#### Connector Part Information

- OEM: 15410450
- Service: 89047131
- Description: 9-Way F Ducon 1.5 (WH)

#### Connector Part Information

- OEM: 12185085
- Service: 88953417
- Description: 9-Way M Ducon 1.5 (WH)

#### Terminal Part Information

- Pins: 2-4, 9
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: 2-4, 9
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X211 Passenger Door Harness to the Body Harness (AU3)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | 2 YE | 443 | Ignition Voltage | 2 | 2 YE | 443 | Ignition Voltage
3 | 0.8 GY | 295 | Door Lock Actuator Lock Control | 3 | 0.8 GY | 295 | Door Lock Actuator Lock Control
4 | 1 BK | 2050 | Ground | 4 | 1 BK | 2050 | Ground
5-8 | -- | -- | Not Used | 5-8 | -- | -- | Not Used
9 | 0.8 TN | 294 | Door Lock Actuator Unlock Control | 9 | 0.8 TN | 294 | Door Lock Actuator Unlock Control

### X275 SIR Coil Harness to the Body Harness

#### Connector Part Information

- OEM: 15336479
- Service: 15306186
- Description: 4-Way F Metri-Pack 280 Series (YE)

#### Connector Part Information

- OEM: 15336476
- Service: 15306363
- Description: 4-Way M Metri-Pack 280 Series (YE)

#### Terminal Part Information

- Pins: A1-A2, B1-B2
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: A1-A2, B1-B2
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X275 SIR Coil Harness to the Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | YE | -- | Steering Wheel Module - Stage 1 - High Control | A1 | 0.5 TN | 3021 | Steering Wheel Module - Stage 1 - High Control
A2 | BN | -- | Steering Wheel Module - Stage 1 - Low Control | A2 | 0.5 BN | 3020 | Steering Wheel Module - Stage 1 - Low Control
B1 | RD | -- | Steering Wheel Module - Stage 2 - High Control | B1 | 0.5 WH | 3023 | Steering Wheel Module - Stage 2 - High Control
B2 | WH | -- | Steering Wheel Module - Stage 2 - Low Control | B2 | 0.5 PK | 3022 | Steering Wheel Module - Stage 2 - Low Control

### X307 Body Harness to the Driver Seat Harness (AG1)

#### Connector Part Information

- OEM: 12059472
- Service: 12101830
- Description: 7-Way F 150, 280 Series GT (BK)

#### Connector Part Information

- OEM: 12052200
- Service: 12117321
- Description: 7-Way M 150, 480 Series Sealed (BK)

#### Terminal Part Information

- Pins: A-D
- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: Pins: A, D: E/1
- Core/Insulation Crimp: Pins: B, C: 2/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

- Pins: G
- Terminal/Tray: 12052139/18
- Core/Insulation Crimp: F/3
- Release Tool/Test Probe: 12094430/J-35616-40 (BU)

#### Terminal Part Information

- Pins: A-D, G
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X307 Body Harness to the Driver Seat Harness (AG1)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 BN | 141 | Ignition Voltage | A | 0.35 BN | 141 | Ignition Voltage
B | 1 OG | 1040 | Battery Positive Voltage | B | 1 OG | 1040 | Battery Positive Voltage
C | 1 BK | 2050 | Ground | C | 1 BK | 2050 | Ground
D | 0.8 OG | 2240 | Battery Positive Voltage | D | 0.8 OG | 2240 | Battery Positive Voltage
E-F | -- | -- | Not Used | E-F | -- | -- | Not Used
G | 3 RD/WH | 1840 | Battery Positive Voltage | G | 3 RD/WH | 1840 | Battery Positive Voltage

### X310 Dome Lamp Harness to the Body Harness

#### Connector Part Information

- OEM: 15318034
- Service: 88987927
- Description: 2-Way F 090 II (WH)

#### Connector Part Information

- OEM: 15427362
- Service: 88987841
- Description: 2-Way M (WH)

#### Terminal Part Information

- Terminal/Tray: 12129960/19
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 12094429/J-35616-18 (BK)

#### Terminal Part Information

- Terminal/Tray: 15305100/19
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 12094429/J-35616-19 (BK)

#### X310 Dome Lamp Harness to the Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 OG | 1732 | Courtesy Lamps Control | 1 | 0.35 OG | 1732 | Courtesy Lamps Control
2 | 0.35 WH | 156 | Courtesy Lamp Low Control | 2 | 0.35 WH | 156 | Courtesy Lamp Low Control

### X311 Body Harness to the Right Rear Passenger Door Harness (Extended Cab)

#### Connector Part Information

- OEM: 12110505
- Service: 15306044
- Description: 2-Way F Metri-Pack 150 Series (YE)

#### Connector Part Information

- OEM: 12160816
- Service: See Catalog
- Description: 2-Way M Metri-Pack 150 Series (YE)

#### Terminal Part Information

- Pins: A-B
- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Terminal Part Information

- Pins: A-B
- Terminal/Tray: 12047581/2
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### X311 Body Harness to the Right Rear Passenger Door Harness (Extended Cab)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 BK/WH | 2118 | Seat Belt Pretensioner - Left - High Control | A | 0.5 BK/WH | 2118 | Seat Belt Pretensioner - Left - High Control
B | 0.5 OG/BK | 2119 | Seat Belt Pretensioner - Left - Low Control | B | 0.5 OG/BK | 2119 | Seat Belt Pretensioner - Left - Low Control

### X312 Body Harness to the Left Rear Passenger Door Harness (Extended Cab)

#### Connector Part Information

- OEM: 12110505
- Service: 15306044
- Description: 2-Way F Metri-Pack 150 Series (YE)

#### Connector Part Information

- OEM: 12160816
- Service: See Catalog
- Description: 2-Way M Metri-Pack 150 Series (YE)

#### Terminal Part Information

- Pins: A-B
- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Terminal Part Information

- Pins: A-B
- Terminal/Tray: 12047581/2
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### X312 Body Harness to the Left Rear Passenger Door Harness (Extended Cab)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 L-GN | 2116 | Seat Belt Pretensioner - Right - High Control | A | 0.5 BK/WH | 2118 | Seat Belt Pretensioner - Right - High Control
B | 0.5 OG | 2117 | Seat Belt Pretensioner - Right - Low Control | B | 0.5 OG/BK | 2119 | Seat Belt Pretensioner - Right - Low Control

### X313 Body Harness to the Passenger Seat Harness

#### Connector Part Information

- OEM: 15332161
- Service: 15306416
- Description: 12-Way F GT 150 Series (BK)

#### Connector Part Information

- OEM: 15332166
- Service: 88953332
- Description: 12-Way M GT 150 Series (BK)

#### Terminal Part Information

- Pins: A-B, D, F-H, J, L-M
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Pins: A-B, D, F-H, J, L-M
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X313 Body Harness to the Passenger Seat Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 D-BU | 2307 | Passenger Air Bag On Indicator Control | A | 0.35 D-BU | 2307 | Passenger Air Bag On Indicator Control
B | 0.35 D-GN | 2308 | Passenger Air Bag Off Indicator Control | B | 0.35 D-GN | 2308 | Passenger Air Bag Off Indicator Control
C | -- | -- | Not Used | C | -- | -- | Not Used
D | 0.35 YE | 1139 | Ignition Voltage | D | 0.35 YE | 1139 | Ignition Voltage
E | -- | -- | Not Used | E | -- | -- | Not Used
F | 0.35 BK/WH | 2151 | Ground | F | 0.35 BK/WH | 2151 | Ground
G | 0.35 RD | 1362 | Seat Belt Switch - Right - Signal | G | 0.35 BK/WH | 2484 | Seat Belt Switch - Right - Signal
H | 0.35 BK | 407 | Low Reference | H | 0.35 BK | 2644 | Low Reference
J | 0.35 L-BU | 5056 | Seat Position Sensor- Right - Signal | J | 0.35 BK | 2645 | Seat Position Sensor- Right - Signal
K | -- | -- | Not Used | K | -- | -- | Not Used
L | 0.35 TN/BK | 371 | Serial Data Link | L | 0.35 PK | 2306 | Serial Data Link
M | 0.35 BK/WH | 2151 | Ground | M | 0.35 BK/WH | 2151 | Ground

### X314 Body Harness to the Driver Seat Harness

#### Connector Part Information

- OEM: 15326815
- Service: 15306396
- Description: 4-Way F GT 150 Series Sealed 4.0 (BK)

#### Connector Part Information

- OEM: 15326820
- Service: 15326820
- Description: 4-Way M GT 150 Series Sealed 4.0 (BK)

#### Terminal Part Information

- Pins: A-D
- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Pins: A-D
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X314 Body Harness to the Driver Seat Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 BK/WH | 238 | Ground | A | 0.35 BK/WH | 238 | Ground (AG1)
B | 0.35 BK/WH | 407 | Seat Belt Switch - Left | B | 0.35 BN/WH | 2151 | Seat Belt Switch - Left (AG1)
C | 0.35 L-GN | 5055 | Seat Position Switch - Left - Signal | C | 0.35 L-GN | 2638 | Seat Position Switch - Left - Signal
D | 0.35 BK | 407 | Low Reference | D | 0.35 TN | 2644 | Low Reference

### X315 Body Harness to the Passenger Seat Harness (AG2)

#### Connector Part Information

- OEM: 15326893
- Service: 89046647
- Description: 5-Way F GT 280 Series (BK)

#### Connector Part Information

- OEM: 15326897
- Service: 88987846
- Description: 5-Way M GT 280 Series

#### Terminal Part Information

- Pins: A-E
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: Pins: B, D-E: 2/A
- Pins: A, C
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Pins: A-E
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X315 Body Harness to the Passenger Seat Harness (AG2)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 BN | 141 | Ignition Voltage | A | 0.35 BN | 141 | Ignition Voltage
B | 1 BK | 2050 | Ground | B | 1 BK | 2050 | Ground
C | 0.35 RD | 1362 | Seat Belt Switch - Right | C | 0.35 L-BU | 2179 | Seat Belt Switch - Right
D | 0.8 OG | 2240 | Battery Positive Voltage | D | 0.8 OG | 2240 | Battery Positive Voltage
E | 1 OG | 1040 | Battery Positive Voltage | E | 1 OG | 1040 | Battery Positive Voltage

### X316 Body Harness to the Left Rear Passenger Door Harness (Crew Cab with A31)

#### Connector Part Information

- OEM: 15427365
- Service: 88953392
- Description: 10-Way F 090 II (WH)

#### Connector Part Information

- OEM: 15427363
- Service: 88953385
- Description: 10-Way M 090 II (WH)

#### Terminal Part Information

- Pins: 1-10
- Terminal/Tray: 12129960/19
- Core/Insulation Crimp: Pins 1-2: A/E/A
- Core/Insulation Crimp: Pins 3-5, 9-10: See Terminal Repair Kit
- Core/Insulation Crimp: Pins 6-8: 6C/A
- Release Tool/Test Probe: 12094429/J-35616-18 (BK)

#### Terminal Part Information

- Pins: 1-10
- Terminal/Tray: 15305100/19
- Core/Insulation Crimp: Pins 1-2: A/E/A
- Core/Insulation Crimp: Pins 3-5, 9-10: See Terminal Repair Kit
- Core/Insulation Crimp: Pins 6-8: C/A
- Release Tool/Test Probe: 12094429/J-35616-19 (BK)

#### X316 Body Harness to the Left Rear Passenger Door Harness (Crew Cab with A31)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 YE | 116 | Left Rear Speaker Output (-) | 1 | 0.5 YE | 116 | Left Rear Speaker Output (-)
2 | 0.5 BN | 199 | Left Rear Speaker Output (+) | 2 | 0.5 BN | 199 | Left Rear Speaker Output (+)
3 | 0.35 D-GN | 168 | Power Window Master Switch Left Rear Up Signal | 3 | 0.35 D-GN | 168 | Power Window Master Switch Left Rear Up Signal
4 | 0.35 YE | 1187 | Power Window Master Switch Left Rear Down Signal | 4 | 0.35 YE | 1187 | Power Window Master Switch Left Rear Down Signal
5 | 0.35 BN | 9 | Park Lamp Control | 5 | 0.35 BN | 9 | Park Lamp Control
6 | 0.8 TN | 294 | Door Lock Actuator Unlock Control (AU3) | 6 | 0.8 TN | 294 | Door Lock Actuator Unlock Control (AU3)
7 | 0.8 GY | 295 | Door Lock Actuator Lock Control (AU3) | 7 | 0.8 GY | 295 | Door Lock Actuator Lock Control (AU3)
8 | 1 BK | 850 | Ground | 8 | 1 BK | 850 | Ground
9 | 0.35 D-BU | 1307 | Power Window Master Switch Lockout Signal | 9 | 0.35 D-BU | 1307 | Power Window Master Switch Lockout Signal
10 | 2 YE | 443 | Ignition Voltage | 10 | 2 YE | 443 | Ignition Voltage

### X316 Body Harness to the Left Rear Passenger Door Harness (Crew Cab without A31)

#### Connector Part Information

- OEM: 15332129
- Service: 15306425
- Description: 2-Way F GT 150 Series (BK)

#### Connector Part Information

- OEM: 15332130
- Service: 88986459
- Description: 2-Way M GT 150 Series (BK)

#### Terminal Part Information

- Pins: A-B
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Pins: A-B
- Terminal/Tray: 15304702/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X316 Body Harness to the Left Rear Passenger Door Harness (Crew Cab without A31)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 YE | 116 | Left Rear Speaker Output (-) | A | 0.5 YE | 116 | Left Rear Speaker Output (-)
B | 0.5 BN | 199 | Left Rear Speaker Output (+) | B | 0.5 BN | 199 | Left Rear Speaker Output (+)

### X316 Body Harness to the Left Rear Passenger Door Harness (Extended Cab)

#### Connector Part Information

- OEM: 12047785
- Service: 12102900
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Connector Part Information

- OEM: 12047786
- Service: 12085536
- Description: 4-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Pins: A-D
- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Terminal Part Information

- Pins: A-D
- Terminal/Tray: 12047581/2
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### X316 Body Harness to the Left Rear Passenger Door Harness (Extended Cab)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 YE | 116 | Left Rear Speaker Output (-) | A | 0.5 YE | 116 | Left Rear Speaker Output (-)
B | 0.5 BN | 199 | Left Rear Speaker Output (+) | B | 0.5 BN | 199 | Left Rear Speaker Output (+)
C | 0.35 GY/BK | 745 | Left Front Door Ajar Switch Signal | C | 0.35 GY/BK | 745 | Left Front Door Ajar Switch Signal
D | 0.35 BK/WH | 1151 | Ground | D | 0.35 BK/WH | 1151 | Ground

### X317 Body Harness to the Right Rear Passenger Door Harness (Crew Cab with A31)

#### Connector Part Information

- OEM: 15427365
- Service: 88953392
- Description: 10-Way F 090 II (WH)

#### Connector Part Information

- OEM: 15427363
- Service: 88953385
- Description: 10-Way M 090 II (WH)

#### Terminal Part Information

- Pins: 1-10
- Terminal/Tray: 12129960/19
- Core/Insulation Crimp: Pins 1-2: A/E/A
- Core/Insulation Crimp: Pins 3-5, 9-10: See Terminal Repair Kit
- Core/Insulation Crimp: Pins 6-8: C/A
- Release Tool/Test Probe: 12094429/J-35616-18 (BK)

#### Terminal Part Information

- Pins: 1-2
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

- Pins: 3-10
- Terminal/Tray: 15305100/19
- Core/Insulation Crimp: Pins 3-5, 9-10: See Terminal Repair Kit
- Core/Insulation Crimp: Pins 6-8 C/A
- Release Tool/Test Probe: 12094429/J-35616-19 (BK)

#### X317 Body Harness to the Right Rear Passenger Door Harness (Crew Cab with A31)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 L-BU | 115 | Right Rear Speaker Output (-) | 1 | 0.5 YE | 115 | Right Rear Speaker Output (-)
2 | 0.5 D-BU | 46 | Right Rear Speaker Output (+) | 2 | 0.5 BN | 46 | Right Rear Speaker Output (+)
3 | 0.35 L-GN | 170 | Power Window Master Switch Right Rear Up Signal | 3 | 0.35 D-GN | 168 | Power Window Master Switch Right Rear Up Signal
4 | 0.35 PU | 171 | Power Window Master Switch Right Rear Down Signal | 4 | 0.35 YE | 1187 | Power Window Master Switch Left Rear Down Signal
5 | 0.35 BN | 9 | Park Lamp Control | 5 | 0.35 BN | 9 | Park Lamp Control
6 | 0.8 TN | 294 | Door Lock Actuator Unlock Control | 6 | 0.8 TN | 294 | Door Lock Actuator Unlock Control
7 | 0.8 GY | 295 | Door Lock Actuator Lock Control | 7 | 0.8 GY | 295 | Door Lock Actuator Lock Control
8 | 1 BK | 2050 | Ground | 8 | 1 BK | 850 | Ground
9 | 0.35 D-BU | 1307 | Power Window Master Switch Lockout Signal | 9 | 0.35 D-BU | 1307 | Power Window Master Switch Lockout Signal
10 | 2 YE | 443 | Ignition Voltage | 10 | 2 YE | 443 | Ignition Voltage

### X317 Body Harness to the Right Rear Passenger Door Harness (Crew Cab without A31)

#### Connector Part Information

- OEM: 15332129
- Service: 15306425
- Description: 2-Way F GT 150 Series (BK)

#### Connector Part Information

- OEM: 15332130
- Service: 88986459
- Description: 2-Way M GT 150 Series (BK)

#### Terminal Part Information

- Pins: A-B
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Pins: A-B
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X317 Body Harness to the Right Rear Passenger Door Harness (Crew Cab without A31)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 L-BU | 115 | Right Rear Speaker Output (-) | A | 0.5 YE | 115 | Right Rear Speaker Output (-)
B | 0.5 D-BU | 46 | Right Rear Speaker Output (+) | B | 0.5 BN | 46 | Right Rear Speaker Output (+)

### X317 Body Harness to the Right Rear Passenger Door Harness (Extended Cab)

#### Connector Part Information

- OEM: 12047785
- Service: 12102900
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Connector Part Information

- OEM: 12047786
- Service: 12085536
- Description: 4-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Pins: A-D
- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Terminal Part Information

- Pins: A-B
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

- Pins: C-D
- Terminal/Tray: 12047581/2
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### X317 Body Harness to the Right Rear Passenger Door Harness (Extended Cab)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 L-BU | 115 | Right Rear Speaker Output (-) | A | 0.5 YE | 115 | Right Rear Speaker Output (-)
B | 0.5 D-BU | 46 | Right Rear Speaker Output (+) | B | 0.5 BN | 46 | Right Rear Speaker Output (+)
C | 0.35 L-GN/BK | 748 | Right Front Door Ajar Switch Signal | C | 0.35 GY/BK | 745 | Right Front Door Ajar Switch Signal
D | 0.35 BK/WH | 1251 | Ground | D | 0.35 BK/WH | 1151 | Ground

### X318 Heat Element to Passenger Seat Harness (AG2)

#### Connector Part Information

- OEM: 12047785
- Service: 12102900
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Connector Part Information

- OEM: 12047786
- Service: 12085536
- Description: 4-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Pins: A-C
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: A-C
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X318 Heat Element to Passenger Seat Harness (AG2)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RD | -- | Battery Positive Voltage | A | OG | 2240 | Battery Positive Voltage
B | BK | -- | Ground | B | BK | 2050 | Ground
C | WH | -- | Passenger Heated Seat High/Low Signal | C | PK | 1501 | Passenger Heated Seat High/Low Signal
D | -- | -- | Not Used | D | -- | -- | Not Used

### X319 Heat Element to Driver Seat Harness (AG1)

#### Connector Part Information

- OEM: 12047785
- Service: 12102900
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Connector Part Information

- OEM: 12047786
- Service: 12085536
- Description: 4-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Pins: A-C
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: A-C
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X319 Heat Element to Driver Seat Harness (AG1)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RD | -- | Battery Positive Voltage | A | OG | 2240 | Battery Positive Voltage
B | BK | -- | Ground | B | BK | 2050 | Ground
C | WH | -- | Driver Heated Seat High/Low Signal | C | PK | 1501 | Driver Heated Seat High/Low Signal
D | -- | -- | Not Used | D | -- | -- | Not Used

### X320 Body Harness to Cargo Lamp/Center High Mounted Stop Lamp (CHMSL) Harness

#### Connector Part Information

- OEM: 15332132
- Service: 88953364
- Description: 3-Way F GT 150 Series (BK)

#### Connector Part Information

- OEM: 15332133
- Service: 88987881
- Description: 3-Way M GT 150 Series (BK)

#### Terminal Part Information

- Pins: A-C
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: Pins A: C/A
- Core/Insulation Crimp: Pins B-C: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Pins: A-C
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X320 Body Harness to Cargo Lamp/Center High Mounted Stop Lamp (CHMSL) Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.8 L-BU | 20 | Stop Lamp Control | A | 0.8 BN | 20 | Stop Lamp Control
B | 0.35 GY/BK | 690 | Courtesy Lamp Control (TR9) | B | 0.35 WH | 690 | Courtesy Lamp Control (TR9)
C | 0.35 BK | 850 | Ground | C | 0.35 BK/WH | 850 | Ground

### X400 Chassis Harness to the License Lamp Harness

#### Connector Part Information

- OEM: 15326801
- Service: 15306156
- Description: 2-Way F GT 150 Series (BK)

#### Connector Part Information

- OEM: 15326806
- Service: 15306166
- Description: 2-Way M 150 Series Sealed (BK)

#### Terminal Part Information

- Pins: A-B
- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Pins: A-B
- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X400 Chassis Harness to the License Lamp Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 BN | 9 | Park Lamp Control | A | 0.5 BN | 9 | Park Lamp Control
B | 0.5 BK | 850 | Ground | B | 0.5 BK | 850 | Ground

### X401 Left Rear Lamp Assembly to the Chassis Harness (without Trailer Accessory)

#### Connector Part Information

- OEM: 15326635
- Service: 88953154
- Description: 6-Way F (BK)

#### Connector Part Information

- OEM: 15326640
- Service: 88953150
- Description: 6-Way M (BK)

#### Terminal Part Information

- Terminal/Tray: 15304719/19
- Core/Insulation Crimp:2/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: 15304731/19
- Core/Insulation Crimp: Pins A-D: E/5
- Core/Insulation Crimp: Pins E: C/5
- Core/Insulation Crimp: Pins F: 2/5
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### X401 Left Rear Lamp Assembly to the Chassis Harness (without Trailer Accessory)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | -- | -- | Not Used | A | 0.5 D-GN | 19 | Right Rear Turn Signal Lamps Control
B | L-GN | -- | Backup Lamp Control | B | 0.5 L-GN | 24 | Backup Lamp Control
C | 0.5 BN | -- | Park Lamp Control | C | 0.5 BN | 9 | Park Lamp Control
D | YE | -- | Left Rear Turn Signal Lamps Control | D | 0.5 YE | 18 | Left Rear Turn Signal Lamps Control
E | L-BU | -- | Stop Lamp Control | E | 0.8 L-BU | 20 | Stop Lamp Control
F | BK | -- | Ground | F | 0.5 BK | 850 | Ground

### X401 Trailer Accessory Harness to the Chassis Harness (UY7)

#### Connector Part Information

- OEM: 15326635
- Service: 88953154
- Description: 6-Way F (BK)

#### Connector Part Information

- OEM: 15326640
- Service: 88953150
- Description: 6-Way M (BK)

#### Terminal Part Information

- Terminal/Tray: 15304719/19
- Core/Insulation Crimp: 2/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: 15304731/19
- Core/Insulation Crimp: Pins A-D: E/5
- Core/Insulation Crimp: Pins E: C/5
- Core/Insulation Crimp: Pins F: 2/5
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### X401 Trailer Accessory Harness to the Chassis Harness (UY7)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | GN | -- | Right Rear Turn Signal Lamps Control | A | 0.5 D-GN | 19 | Right Rear Turn Signal Lamps Control
B | BK | -- | Backup Lamp Control | B | 0.5 L-GN | 24 | Backup Lamp Control
C | BN | -- | Park Lamp Control | C | 0.5 BN | 9 | Park Lamp Control
D | YE | -- | Left Rear Turn Signal Lamps Control | D | 0.5 YE | 18 | Left Rear Turn Signal Lamps Control
E | BU | -- | Stop Lamp Control | E | 0.8 L-BU | 20 | Stop Lamp Control
F | WH | -- | Ground | F | 0.8 BK | 850 | Ground

### X402 Right Rear Lamp Assembly to the Chassis Harness

#### Connector Part Information

- OEM: 15326822
- Service: 88987186
- Description: 5-Way F GT 150 Series Sealed 4.0 (BK)

#### Connector Part Information

- OEM: 15326827
- Service: 89046648
- Description: 5-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: 2/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: Pins: A-C, E: E/4
- Core/Insulation Crimp: Pins D: E/1
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X402 Right Rear Lamp Assembly to the Chassis Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | L-GN | -- | Backup Lamp Control | A | 0.5 L-GN | 24 | Backup Lamp Control
B | BN | -- | Park Lamp Control | B | 0.5 BN | 9 | Park Lamp Control
C | D-GN | -- | Right Rear Turn Signal Lamps Control | C | 0.5 D-GN | 19 | Right Rear Turn Signal Lamps Control
D | L-BU | -- | Stop Lamp Control/Stop Lamp Switch Signal | D | 0.8 L-BU | 20 | Stop Lamp Control/Stop Lamp Switch Signal
E | BK | -- | Ground | E | 0.5 BK | 850 | Ground

### X403 Left Rear Lamp Assembly to the Trailer Accessory Harness (Trailer Accessory)

#### Connector Part Information

- OEM: 15326635
- Service: 88953154
- Description: 6-Way F (BK)

#### Connector Part Information

- OEM: 15326640
- Service: 88953150
- Description: 6-Way M (BK)

#### Terminal Part Information

- Terminal/Tray: 15304719/19
- Core/Insulation Crimp: 2/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: 15304731/19
- Core/Insulation Crimp: Pins A-D: E/5
- Core/Insulation Crimp: Pins E: C/5
- Core/Insulation Crimp: Pins F: 2/5
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### X403 Left Rear Lamp Assembly to the Trailer Accessory Harness (UY7)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | -- | -- | Not Used | A | GN | -- | Right Rear Turn Signal Lamps Control
B | L-GN | -- | Backup Lamp Control | B | BK | -- | Backup Lamp Control
C | BN | -- | Park Lamp Control | C | BN | -- | Park Lamp Control
D | YE | -- | Left Rear Turn Signal Lamps Control | D | YE | -- | Left Rear Turn Signal Lamps Control
E | L-BU | -- | Stop Lamp Control | E | BU | -- | Stop Lamp Control
F | BK | -- | Ground | F | WH | -- | Ground

### X404 (UY7) Chassis Harness to License Lamp Harness

#### Connector Part Information

- OEM: 12052613
- Service: 12085212
- Description: 2-Way F Metri-Pack 480 Series Sealed (BK)

#### Connector Part Information

- OEM: 12052172
- Service: See Catalog
- Description: 2-Way M Metri-Pack 480 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12052139/18
- Core/Insulation Crimp: F/3
- Release Tool/Test Probe: 12094430/J-35616-40 (BU)

#### Terminal Part Information

- Pin: A
- Terminal/Tray: 12052172/18
- Core/Insulation Crimp: F/3

#### X404 (UY7) Chassis Harness to License Lamp Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 3 RD | 742 | Battery Positive Voltage | A | 3 RD/BK | 742 | Battery Positive Voltage
B | -- | -- | Not Used | B | -- | -- | Not Used