For 1990-2009 cars

## Endgate Emblem/Nameplate Replacement OLD

#### Tools Required

J 25070 Heat Gun

### Removal Procedure

Important: Use the tape for protection and alignment marks for alignment of the new emblem.

1. Apply tape to the area around the tailgate emblem.
2. Heat the emblem/nameplate, using a J 25070 , 152 mm (6 in) from the surface.
3. Apply the heat using a circular motion for about 30 seconds.

Notice: Use a plastic, flat-bladed tool to prevent paint damage when removing an emblem/name plate.

4. Remove the emblem/nameplate from the tailgate surface using a plastic, flat-bladed tool.
5. Remove all adhesive from the tailgate panel surface and the back of the emblem/nameplate using 3M™ scotch brite molding adhesive remover disk 3M™ P/N 07501 or equivalent.
6. Clean the tailgate surface using varnish makers and painters (VMP) naphtha.

### Installation Procedure

1. If the location of the emblem/nameplate has not been marked, apply tape and use the following dimensions:

• | Dimension (a) is 59.5 mm (2.34 in) from the edge of the tailgate to the emblem/nameplate.

• | Dimension (b) is 12.1 mm (0.48 in) from the bottom of the tailgate to the emblem/nameplate.

• | Dimension (c) is 5.1 mm (0.2 in) from the bottom of the tailgate to the emblem/nameplate.

• | Dimension (d) is 59.4 mm (2.34 in) from the edge of the tailgate to the emblem/nameplate.

2. Warm the tailgate surface with a J 25070 , 152 mm (6 in) from the surface to a minimum of 21°C (70°F).

Important: Do not touch the adhesive backing of the emblem/nameplate.

3. Remove the backing from the front end of the emblem/nameplate.
4. Press the emblem/nameplate to the tailgate surface while continuing to remove the backing.
5. Hand roll the emblem/nameplate to the tailgate panel to ensure proper adhesion.
6. Inspect the emblem/nameplate for bonding.
7. Remove the tape from the area around the emblem/nameplate.

## Endgate Emblem/Nameplate Replacement OLD

#### Tools Required

J 25070 Heat Gun

### Removal Procedure

Important: Use the tape for protection and alignment marks for alignment of the new emblem.

1. Apply tape to the area around the tailgate emblem.
2. Heat the emblem/nameplate, using a J 25070 , 152 mm (6 in) from the surface.
3. Apply the heat using a circular motion for about 30 seconds.

Notice: Use a plastic, flat-bladed tool to prevent paint damage when removing an emblem/name plate.

4. Remove the emblem/nameplate from the tailgate surface using a plastic, flat-bladed tool.
5. Remove all adhesive from the tailgate panel surface and the back of the emblem/nameplate using 3M™ scotch brite molding adhesive remover disk 3M™ P/N 07501 or equivalent.
6. Clean the tailgate surface using varnish makers and painters (VMP) naphtha.

### Installation Procedure

1. If the location of the emblem/nameplate has not been marked, apply tape and use the following dimensions:

• | Dimension (a) is 61 mm (2.4 in) from the edge of the tailgate to the emblem/nameplate.

• | Dimension (b) is 66.4 mm (2.61 in) from the bottom of the tailgate to the emblem/nameplate.

2. Warm the tailgate surface with a J 25070 , 152 mm (6 in) from the surface to a minimum of 21°C (70°F).

Important: Do not touch the adhesive backing of the emblem/nameplate.

3. Remove the backing from the front end of the emblem/nameplate.
4. Press the emblem/nameplate to the tailgate surface while continuing to remove the backing.
5. Hand roll the emblem/nameplate to the tailgate panel to ensure proper adhesion.
6. Inspect the emblem/nameplate for bonding.
7. Remove the tape from the area around the emblem/nameplate.