For 1990-2009 cars

### Removal Procedure

Caution: Refer to Brake Dust Caution in the Preface section.

Caution: Refer to Brake Fluid Irritant Caution in the Preface section.

1. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation .
2. Remove the brake hose from the brake caliper.

Important: When removing the brake hose bolt from the brake caliper, ensure that the copper gaskets are not stuck to the brake caliper or the brake hose.

3. Remove the copper gaskets from the brake hose and bolt.
4. Discard the copper gaskets. DO NOT reuse them, replace with NEW copper gaskets.
5. Using a rubber plug or equivalent, plug the end of the brake hose to prevent excessive brake fluid loss and contamination.
6. Remove the brake caliper slide pin bolts.
7. Remove the brake caliper from the mounting bracket.

### Installation Procedure

1. Position the brake caliper assembly on the mounting bracket.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the guide pin bolts.

Tighten
Tighten the guide pin bolts to 40 N·m (29 lb ft).

3. Remove the rubber plugs from the brake hose.
4. Install the NEW copper gaskets and bolt on the brake hose.
5. Install the brake hose on the brake caliper.

Tighten
Tighten the brake hose bolt to 40 N·m (29 lb ft).

6. Bleed the system. Refer to Hydraulic Brake System Bleeding .
7. Install the tire and wheel. Refer to Tire and Wheel Removal and Installation .
8. Lower the vehicle.