For 1990-2009 cars

Table 1: | Indicators
Table 2: | DIC Warning Messages

#### Indicators

Symbol | Reference
--- | ---
| ABS: Refer to ABS Description and Operation
| Air Bag: Refer to SIR System Description and Operation
(Canada) BRAKE (U.S.) | Brake: Refer to Brake Warning System Description and Operation
| Charge: Refer to Charging System Description and Operation
(Canada) CRUISE (U.S.) | CRUISE: Refer to Cruise Control Description and Operation
| Fasten Safety Belt: Refer to Seat Belt System Description and Operation
| Fasten Passenger Seat Belts: Refer to Seat Belt System Description and Operation
| High Beam: Refer to Exterior Lighting Systems Description and Operation
| Passenger Air Bag Off: Refer to SIR System Description and Operation
| Passenger Air Bag On: Refer to SIR System Description and Operation
(Canada) SECURITY (U.S.) | SECURITY: Refer to Content Theft Deterrent (CTD) Description and Operation
(Canada) SERVICE ENGINE SOON (U.S.) | Refer to:

• | Powertrain Control Module Description for the 2.9L engine

• | Powertrain Control Module Description for the 3.7L engine

| Tire Pressure Monitor: Refer to Tire Pressure Monitor Description and Operation
| Turn Signals: Refer to Exterior Lighting Systems Description and Operation

#### DIC Warning Messages

Message | Reference
--- | ---
ABS | Refer to ABS Description and Operation
A/C OFF | Refer to Air Temperature Description and Operation
BATTERY | Refer to Charging System Description and Operation
BRAKE FLUID | Refer to Brake Warning System Description and Operation
BRAKE SYSTEM | Refer to Brake Warning System Description and Operation
CARGO LAMP | Refer to Interior Lighting Systems Description and Operation
CHANGE OIL | The instrument panel cluster (IPC) illuminates the CHANGE OIL indicator when the powertrain control module (PCM) determines that the engine oil should be changed. Refer to GM Oil Life System Resetting .
CHECK FUEL CAP | The IPC illuminates the CHECK FUEL CAP message in the driver information center (DIC) when the PCM detects a low fuel pressure condition.
DOORS | Refer to Door Ajar Indicator Description and Operation
DOME LAMP | Refer to Interior Lighting Systems Description and Operation
ENG HOT | Refer to Cooling System Description and Operation
LOW FUEL | The IPC illuminates the LO FUEL message in the DIC when the IPC detects that the fuel level is less than a pre-determined value.
LOW TRAC | Refer to ABS Description and Operation
MAP LAMP | Refer to Interior Lighting Systems Description and Operation
OIL | The IPC illuminates the OIL message in the DIC when the PCM detects a low oil pressure condition.
OIL LIFE | The IPC illuminates the OIL LIFE message when the PCM determines that the engine oil should be changed.
PARK BRAKE | Refer to Park Brake System Description and Operation
REDUCED POWER | Refer to:

• | Powertrain Control Module Description for the 2.9L engine

• | Powertrain Control Module Description for the 3.7L engine

SERV 4WD | Refer to Transfer Case Description and Operation
SERV VEH | Refer to:

• | Powertrain Control Module Description for the 2.9L engine

• | Powertrain Control Module Description for the 3.7L engine

SERVICE TRACTION | Refer to ABS Description and Operation
TRAC OFF | Refer to ABS Description and Operation