For 1990-2009 cars

1. Remove the following parts:

1.1. | Hex head nut (90)

1.2. | Manual valve link (89)

1.3. | Detent lever (88)

1.4. | Parking lock actuator assembly (85)

1.5. | Manual shaft retainer (83)

1.6. | Manual shaft (84)

2. Remove the manual shaft seal (82) with a screwdriver.
3. Remove the following components:

3.1. | The parking lock bracket bolt (87)

3.2. | The parking lock bracket (86)