For 1990-2009 cars

### Removal Procedure

1. Remove the screws retaining the instrument panel (I/P) compartment assembly to the I/P.
2. Open the I/P compartment door.
3. Remove the I/P compartment assembly from the vehicle.

### Installation Procedure

1. Position the I/P compartment assembly to the I/P.
2. Close and fully latch the I/P compartment door.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the fasteners retaining the I/P compartment assembly to the I/P. Tighten the fasteners to 3 N·m (27 lb in).
4. Ensure the alignment of the door allows for proper operation.