For 1990-2009 cars

### Removal Procedure

1. Remove the front bumper. Refer to Front Bumper Replacement .
2. Remove the right tow hook nuts and bolts from the frame rail.
3. Remove the right tow hook from the vehicle.
4. Remove the left tow hook nuts and bolts from the frame rail.
5. Remove the left tow hook from the vehicle.

### Installation Procedure

1. Install the left tow hook to the frame rail.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the nuts and the bolts to the frame rail.

Tighten
Tighten the bolts to 100 N·m (74 lb ft).

3. Install the left tow hook to the frame rail.
4. Install the nuts and the bolts to the frame rail.

Tighten
Tighten the bolts to 100 N·m (74 lb ft).

5. Install the front bumper. Refer to Front Bumper Replacement .