For 1990-2009 cars

### Removal Procedure

Caution: Refer to Approved Equipment for Collision Repair Caution in the Preface section.

1. Locate and drill out the spot welds.
2. Remove the tie down loop.

### Installation Procedure

1. Prepare all mating surfaces as necessary.
2. Apply GM-approved Weld-Thru coating or equivalent to all mating surfaces. Refer to Anti-Corrosion Treatment and Repair .
3. Position the tie down loop.
4. Plug weld accordingly.
5. Clean and prepare all welded surfaces.
6. Apply the sealers and anti-corrosion materials to the repair area, as necessary. Refer to Anti-Corrosion Treatment and Repair .
7. Paint and repair the area. Refer to Basecoat/Clearcoat Paint Systems .