For 1990-2009 cars

## Shift Lever Assembly Replacement w/o D06

### Removal Procedure

1. Pull upward on the front of the boot (3) in order to disengage the boot retainers (2) from the floor console (1).
2. Remove the set screw (1) from the shift lever (2).
3. Remove the shift lever assembly from the control lever.

### Installation Procedure

1. Install the shift lever assembly to the control lever, aligning the set screw threaded hole with the seat (3)
2. Apply threadlock GM P/N 12345493 (Canadian P/N 10953488) to the shift lever set screw threads.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the shift lever set screw and tighten to 25 N·m (18 lb ft).
4. Position the boot tabs (4) under the rear of the console opening.
5. Push downward on the front of the boot (3) in order to engage the boot retainers (2) with the floor console (1).

## Shift Lever Assembly Replacement D06

### Removal Procedure

1. Pull upward on the boot (1) in order to disengage the bezel retainers (2) from the console (3).
2. Remove the set screw (1) from the shift lever (2).
3. Remove the shift lever assembly from the control lever.

### Installation Procedure

1. Install the shift lever assembly to the control lever, aligning the set screw threaded hole with the seat (3).
2. Apply threadlock GM P/N 12345493 (Canadian P/N 10953488) to the shift lever set screw threads.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the shift lever set screw and tighten to 25 N·m (18 lb ft).
4. Push downward on the bezel in order to engage the bezel retainers (2) with the console (3).