For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
3. Remove the front outside door handle. Refer to Front Side Door Outside Handle Replacement .
4. Remove the bolts retaining the lock cylinder to the front outside door handle.
5. Remove the lock cylinder from the door.

### Installation Procedure

1. Install the lock cylinder to the front outside door handle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts retaining the lock cylinder to the outside door handle.

Tighten
Tighten the lock cylinder bolts to 9 N·m (80 lb in).

3. Install the front outside door handle. Refer to Front Side Door Outside Handle Replacement .
4. Install the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
5. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement .