For 1990-2009 cars

## Power Steering Fluid Reservoir Replacement LH8

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the power steering pump. Refer to Power Steering Pump Replacement.

1 | Power Steering Fluid Reservoir Bracket Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m (18 lb ft)
2 | Power Steering Fluid Reservoir Bracket
3 | Power Steering Fluid Reservoir Retainer (Qty: 2)
4 | Power Steering Fluid Reservoir Tip Transfer any parts as needed.