For 1990-2009 cars

## Power Steering Pump Pulley Replacement LLV, LLR

### Tools Required

• | J 25033-C Power Steering Pump Pulley Installer

• | J 25034-C Power Steering Pump Pulley Remover

### Removal Procedure

1. Remove the drive belt. Refer to Drive Belt Replacement for the 2.9L engine or Drive Belt Replacement for the 3.7L engine.
2. Remove the power steering pump pulley using J 25034-C .
3. Remove the pulley from the pump shaft.

### Installation Procedure

1. Install the power steering pump pulley to the end of the power steering pump shaft.
2. Install the power steering pump pulley to the power steering pump using J 25033-C .
3. Install the power steering pump pulley (1) flush against the end of the power steering pump shaft (2), with an allowable variance of 0.25 mm (0.010 in).
4. Install the drive belt. Refer to Drive Belt Replacement for the 2.9L engine or Drive Belt Replacement for the 3.7L engine.

## Power Steering Pump Pulley Replacement LH8

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the accessory drive belt. Refer to Drive Belt Replacement - Accessory .

1 | Power Steering Pump Pulley

#### Procedure

1. Use remover J 25034-C to remove the power steering pump pulley.
2. Use installer J 25033-C to install the power steering pump pulley.
3. Ensure the axial tolerance of the power steering pulley on the shaft is within 0.25 mm (0.010 in).

#### Special Tools

• | J 25033-C Pulley Installer

• | J 25034-C Pulley Remover