For 1990-2009 cars

### Removal Procedure

1. Disconnect the stop lamp switch electrical connectors (1).
2. Rotate the switch counterclockwise.
3. Remove the switch from the bracket.
4. Remove the switch from the vehicle.

### Installation Procedure

1. Position the switch near the bracket.
2. Ensure the switch key-way is properly indexed to the plastic retainer.
3. Install and adjust the switch. Refer to Stop Lamp Switch Adjustment .
4. Connect the stop lamp switch electrical connectors (1).
5. Check the switch for proper operation.