For 1990-2009 cars

1. Install the timing chain tensioner.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the timing chain tensioner bolts and tighten to 25 N·m (18 lb ft).
3. Install the timing chain tensioner guide.
4. Install the timing chain tensioner guide bolts and tighten to 22 N·m (16 lb ft).
5. Install the timing chain tensioner shoe.
6. Install the timing chain tensioner shoe bolt and tighten to 25 N·m (18 lb ft).
7. Install the cylinder head access hole plugs and tighten to 5 N·m (44 lb in).