For 1990-2009 cars

### Removal Procedure

Warning: Refer to Brake Dust Warning in the Preface section.

1. Within the engine compartment, disconnect the wheel speed sensor electrical connector (1).
2. Release the wheel speed sensor harness connector from the wheelhouse.
3. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
4. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
5. Release the wheel speed sensor harness clips (1) from the suspension upper control arm.
6. Release the wheel speed sensor harness grommet (1) from the mounting bracket.
7. Remove the wheel speed sensor harness bracket bolt (1).
8. Thoroughly clean the wheel speed sensor mounting area of the steering knuckle of any dirt and debris.
9. Remove the wheel speed sensor bolt (1).

Note: Do not pry or lever against the wheel speed sensor to remove.

10. Carefully remove the wheel speed sensor from the suspension knuckle by pulling straight upward.

### Installation Procedure

1. Install the wheel speed sensor to the suspension knuckle.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the wheel speed sensor bolt (1) and tighten to 8 N·m (71 lb in).
3. Install the wheel speed sensor harness bracket bolt (1) and tighten to 9 N·m (80 lb in).
4. Install the wheel speed sensor harness grommet (1) to the mounting bracket.
5. Install the wheel speed sensor harness clips (1) to the suspension upper control arm.
6. Install the wheel speed sensor harness connector to the wheelhouse.
7. Connect the wheel speed sensor electrical connector (1).
8. Install the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
9. Perform the Diagnostic System Check - Vehicle.