For 1990-2009 cars

#### Tools Required

J 9886-01 Door Handle Clip Remover or equivalent

### Removal Procedure

1. Open the front and rear side access door.
2. Remove the spring clip retaining the rear side access door handle by inserting J 9886-01 between the door handle, and the door, and pressing the spring clip off the door handle.
3. Remove the rear side access door handle from the door.

### Installation Procedure

1. Install the spring clip onto the rear side access door handle.
2. Install the rear side access door handle onto the rear side access door control assembly.
3. Press the handle in until the spring clip retaining the handle is fully seated.