For 1990-2009 cars

### Removal Procedure

1. Using a flat-bladed plastic tool, carefully release the 4 tabs (1) retaining the air outlet assembly to the instrument panel (I/P).
2. Remove the air outlet assembly from the I/P
3. If replacing the vent assembly or the bezel, separate the bezel from the vent assembly by carefully releasing the 4 retaining tabs.

### Installation Procedure

1. If replacing the vent assembly or the bezel, install the bezel to the vent assembly by seating the 4 retaining tabs.
2. Install the air outlet assembly to the I/P ensuring the retaining tabs are fully seated.