For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
Accelerator Pedal Position (APP) Sensor Nut | 9 N·m | 80 lb in
Air Cleaner Housing Integral Bolt | 15 N·m | 11 lb ft
Air Cleaner Outlet Duct Clamp | 3.5 N·m | 31 lb in
Camshaft Position (CMP) Sensor/Wire Harness Bolt | 12 N·m | 106 lb in
Crankshaft Position (CKP) Sensor Bolt | 25 N·m | 18 lb ft
Engine Coolant Temperature (ECT) Sensor | 20 N·m | 15 lb ft
Engine Wiring Harness Bracket Nut | 9 N·m | 80 lb in
Evaporative Emission (EVAP) Canister Bolt | 25 N·m | 18 lb ft
Fuel Feed and EVAP Line Bracket Bolt | 10 N·m | 89 lb in
Fuel Feed Line to Fuel Tank Module Fitting | 30 N·m | 22 lb ft
Fuel Fill Hose Clamp | 2.5 N·m | 22 lb in
Fuel Fill Pipe Bracket Nut | 10 N·m | 89 lb in
Fuel Fill Hose Ground Strap Bolt | 9 N·m | 80 lb in
Fuel Pipe Bracket Bolt | 4.5 N·m | 40 lb in
Fuel Pipe Bracket to Transmission Stud Nut | 9 N·m | 80 lb in
Fuel Rail Bolt | 10 N·m | 89 lb in
Fuel Rail Retainer Clip Screw | 3.8 N·m | 34 lb in
Fuel Tank Shield Bolt | 10 N·m | 89 lb in
Fuel Tank Strap Bolt | 32 N·m | 24 lb ft
Heated Oxygen Sensor (HO2S) | 42 N·m | 31 lb ft
Ignition Coil Bolt | 8 N·m | 71 lb in
Knock Sensor (KS) Bolt | 20 N·m | 15 lb ft
Mass Airflow/Intake Air Temperature (MAF/IAT) Sensor Screw | 1.5 N·m | 13 lb in
Spark Plug | 20 N·m | 15 lb ft
Throttle Body Bolt | 10 N·m | 89 lb in