For 1990-2009 cars

### Removal Procedure

1. Open the front door.

Remove the bolt retaining the front door check link to the body.

3. Remove the front door wiring harness grommet from the body and disconnect the door wiring harness connectors. Refer to Front Side Door Wiring Harness Replacement.
4. Remove the bolts (1) retaining the front door hinge keeper straps.
5. With the aid of an assistant, lift the front door up off the body side hinges and place the door on a clean, protected surface.
6. Remove the bolts retaining the door side hinges to the door.
7. Remove the hinges from the door.

### Installation Procedure

1. Position the door side front door hinge to the door.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the bolts retaining the door side door hinge to the door and tighten to 27 N·m (20 lb ft).
3. With the aid of an assistant, lower the front door down onto the body side hinge straps.
4. Install the bolts (1) retaining the front door hinge keeper straps and tighten to 25 N·m (18 lb ft).
5. Connect the front door wiring harness connectors and install the front door wiring harness grommet to the body. Refer to Front Side Door Wiring Harness Replacement.
6. Install the bolt retaining the front door check link to the body and tighten to 25 N·m (18 lb ft).
7. Inspect the door for proper operation and alignment. Refer to Front Side Door Adjustment.