For 1990-2009 cars

### Replacement Procedure

1. Release the park brake.
2. Raise the vehicle. Refer to Lifting and Jacking the Vehicle .
3. Remove the park brake adjusting nut.
4. Remove the front park brake cable from the equalizer.
5. Remove the right rear park brake cable from the equalizer.
6. Remove the left rear park brake cable from the equalizer.
7. Remove the equalizer.

### Installation Procedure

1. Install the left rear park brake cable in the equalizer.
2. Install the right rear park brake cable in the equalizer.
3. Install the front park brake cable in the equalizer.
4. Install the park brake cable adjusting nut.
5. Adjust the park brake cable. Refer to Park Brake Adjustment .
6. Lower the vehicle.