For 1990-2009 cars

1. Install the timing chain tensioner.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the timing chain tensioner bolts. Tighten the timing chain tensioner bolts to 25 N·m (18 lb ft).
3. Install the timing chain tensioner guide.
4. Install the timing chain tensioner guide bolts. Tighten the timing chain tensioner guide bolts to 22 N·m (16 lb ft).
5. Install the timing chain tensioner shoe.
6. Install the timing chain tensioner shoe bolt. Tighten the timing chain tension shoe bolt to 25 N·m (18 lb ft).
7. Install the cylinder head access hole plugs. Tighten the cylinder head access hole plugs to 5 N·m (44 lb in).