For 1990-2009 cars

### Removal Procedure

1. Remove the fuel line clip (1) from the oil level indicator bracket.
2. Pull the oil level indicator from the tube.
3. Remove the oil level indicator tube bolt.
4. Remove the oil level indicator tube from the engine oil pan.

### Installation Procedure

1. Lightly lubricate the O-ring seal with clean engine oil.
2. Install the oil level indicator tube into the engine oil pan.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the oil level indicator tube bolt.

Tighten
Tighten the bolt to 10 N·m (89 lb in).

4. Install the oil level indicator into the tube.
5. Install the fuel line clip (1) to the oil level indicator bracket.