For 1990-2009 cars

Description of Usage | Ref No.* | Qty | Size | Specification
--- | --- | --- | --- | ---
Metric | English
Accumulator Cover to Case | 58 | 1 | M6x1.0x65 | 8-14 N·m | 71-124 lb in
Accumulator Cover to Case | 117 | 1 | M6x1.0x65 | 8-14 N·m | 71-124 lb in
Accumulator Cover to Case | 118 | 2 | M6x1.0x28.0 | 8-14 N·m | 71-124 lb in
Accumulator Cover to Case | 59 | 2 | M6x1.0x35 | 8-14 N·m | 71-124 lb in
Control Lever Nut | -- | -- | -- | 20 N·m | 15 lb ft
Converter Cover Bolt | -- | -- | -- | 10 N·m | 89 lb in
Converter Housing to Case | 94 | 8 | M10x1.5gx45 | 65-75 N·m | 48-55 lb ft
Cooler Pipe Connector | 95 | 2 | 1/4-18NSPS(SPL) | 35-41 N·m | 26-30 lb ft
Detent Spring to Valve Body | 64 | 1 | M8x1.25x20 | 20-27 N·m | 15-20 lb ft
Converter Housing to Case Screw | -- | -- | -- | 65.0-75.0 N·m | 48-55 lb ft
Extension Housing to Case | 32 | 6 | M10x1.5x33.4 | 42-48 N·m | 31-35 lb ft
Extension Housing to Case (4WD Shipping) | N/A | 4 | M10x1.5x33.4 | 11-23 N·m | 8-17 lb in
Filler Tube Nut | -- | -- | -- | 12.5 N·m | 111 lb in
Floorshift Control Bolt | -- | -- | -- | 10 N·m | 89 lb in
Forward Accumulator Cover to Valve Body | 364 | 3 | M6x1.0x17.7 | 8-14 N·m | 71-124 lb in
Fuel Hose Pipe Bracket Nut | -- | -- | -- | 20 N·m | 15 lb ft
Heat Shield to Transmission Bolt | -- | -- | -- | 17 N·m | 13 lb ft
Input Speed Sensor Hole Plug to Pump Cover | 248 | 1 | M6x1.0x17.7 | 9-11 N·m | 80-97 lb in
Input Speed Sensor to Pump Cover | 247 | 1 | M6x1.0x17.7 | 9-11 N·m | 80-97 lb in
Line Pressure Test Hole Plug | 39 | 1 | 1/8-27NPTF | 8-14 N·m | 71-124 lb in
Negative Battery Cable Bolt | -- | -- | -- | 15 N·m | 11 lb ft
Oil Cooler Pipe Fitting | 10 | 2 | 9/16-18UNF | 20 +/- 2 N·m | 15 lb ft
Oil Level Indicator Bolt | -- | -- | -- | 47 N·m | 35 lb ft
Oil Passage Cover (Spacer Plate Support) to Case | 77 | 3 | M6x1.0x17.7 | 8-14 N·m | 71-124 lb in
Oil Passage Cover (Spacer Plate Support) to Case | 115 | 1 | M6x1.0x19.0 | 8-14 N·m | 71-124 lb in
Park Lock Bracket to Case | 87 | 1 | M8x1.25x20 | 27-34 N·m | 20-25 lb ft
Park/Neutral Back Up Switch Bolt | -- | -- | -- | 27 N·m | 20 lb ft
Park/Neutral Position Switch Screw | -- | -- | -- | 3 N·m | 27 lb in
Plate to Case (Shipping) | N/A | 2 | M10x1.5x35 | 27-34 N·m | 20-25 lb ft
Plate to Converter (Shipping) | N/A | 1 | M10x1.5x25 | 27-34 N·m | 20-25 lb ft
Plate to Converter (Shipping) | N/A | 1 | M10x1.5x15 | 27-34 N·m | 20-25 lb ft
Pressure Control Solenoid Bracket to Valve Body Bolt | 364 | 1 | M6x1.0x17.7 | 8-14 N·m | 71-124 lb in
Pump Assembly to Case | 2 | 7 | M8x1.25x60 | 26-32 N·m | 19-24 lb ft
Pump Cover to Pump Body | 233 | 5 | M8x1.25x40 | 20-27 N·m | 15-20 lb ft
Shift Cable Grommet Screw | -- | -- | -- | 1.7 N·m | 15 lb in
Shift Control Cable Attachment | -- | -- | -- | 20 N·m | 15 lb ft
Speed Sensor Retainer Bolt | 35 | 1 | M6x1.0x15 | 10.5-13.5 N·m | 93-119 lb in
TCC Solenoid Assembly to Case | 68 | 2 | M6x1.0x12 | 8-14 N·m | 71-124 lb in
Torque Converter Bolt | -- | -- | -- | 60 N·m | 44 lb ft
Transmission Oil Pan to Case Screw | 76 | 16 | M8x1.25x19.3 | 9.5-13.6 N·m | 84-120 lb in
Transmission Mount to Transmission Bolt | -- | -- | -- | 60 N·m | 44 lb ft
Transmission Mount to Transmission Support Nut | -- | -- | -- | 57 N·m | 42 lb ft
Transmission Mounting Bolt | -- | -- | -- | 50 N·m | 37 lb ft
Transmission Range Selector Cable Bracket Bolt | -- | -- | -- | 25 N·m | 18 lb ft
Transmission to Engine Bolt | -- | -- | -- | 47 N·m | 35 lb ft
Valve Body to Case | 120 | 3 | M6x1.0x54.4 | 8-14 N·m | 71-124 lb in
Valve Body to Case | 62 | 12 | M6x1.0x47.5 | 8-14 N·m | 71-124 lb in
Valve Body to Case | 59 | 2 | M6x1.0x35 | 8-14 N·m | 71-124 lb in
* Reference Number refers to the callout number on the disassembled view.