For 1990-2009 cars

### Removal Procedure

1. If equipped, tilt the steering wheel to the full down position.
2. If equipped with a steering column mounted shift lever, block the wheels and position the shift lever in FIRST gear.
3. Carefully release the clips retaining the bezel to the instrument panel (I/P).
4. Remove the bezel from the I/P.

### Installation Procedure

1. Position the bezel to the I/P.
2. Install the bezel, ensuring the retaining clips are fully seated.
3. If equipped with tilt steering, return the steering wheel to a neutral position.