For 1990-2009 cars

### Removal Procedure

1. Remove the seat from the vehicle. Refer to Front Seat Replacement - Bucket or Split Bench Seat Replacement.
2. Disconnect the seat belt buckle electrical connector (1).
3. Remove the bolt (2) securing the seat belt buckle assembly (1) to the seat adjuster.
4. Pull the seat belt buckle assembly (1) out though the opening in the seat cushion.

### Installation Procedure

1. Install the seat belt buckle assembly (1) through the seat cushion pad.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the seat belt buckle assembly (1) to the seat adjuster with the bolt (2).

Tighten
Tighten the front seat belt buckle bolt to 55 N·m (41 lb ft).

3. Connect the seat belt buckle electrical connector (1).
4. Install the seat from the vehicle. Refer to Front Seat Replacement - Bucket or Split Bench Seat Replacement.