For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Body Side Front Door Bolts | 27 N·m | 20 lb ft
Body Side Rear Door Hinge Bolts | 25 N·m | 18 lb ft
Door Side Front Door Hinge Bolts | 27 N·m | 20 lb ft
Door Side Rear Door Hinge Bolts | 25 N·m | 18 lb ft
Endgate to Body Hinge Bolts | 20 N·m | 15 lb ft
Front Door Check Link Bolts | 25 N·m | 18 lb ft
Front Door Check Link Nuts | 9 N·m | 90 lb in
Front Door Hinge Bolts | 25 N·m | 18 lb ft
Front Fender Bolts | 10 N·m | 89 lb in
Fuel Filler Door Screws | 5 N·m | 44 lb in
Fuel Filler Pocket Screws | 10 N·m | 89 lb in
Hinge Keeper Strap Bolts | 25 N·m | 18 lb ft
Hood Hinge Bolts | 25 N·m | 18 lb ft
Hood Latch Bolts | 10 N·m | 89 lb in
Hood Latch Support Bolts | 10 N·m | 89 lb in
Pickup Box to Frame Rail Bolts | 85 N·m | 63 lb ft
Prop Pod Bolt | 10 N·m | 89 lb in
Rear Door Check Link Bolt | 25 N·m | 18 lb ft
Rear Door Check Link Nuts | 9 N·m | 80 lb in
Rear Side Access Check Link Nuts | 9 N·m | 80 lb in
Rear Side Access Door Hinge Bolts | 25 N·m | 18 lb ft
Release Handle to the Knee Bolster Screws | 1 N·m | 9 lb in