For 1990-2009 cars

### Removal Procedure

1. Raise and support the hood.
2. Remove the washer hose from the nozzles. Refer to Washer Nozzle Replacement .
3. Remove the hose from the air inlet panel.
4. Disconnect the hose (1) from the washer pump.
5. Install a cap on the washer pump outlet in order to prevent excessive washer solvent loss.
6. Remove the washer hose from the vehicle.

### Installation Procedure

1. Position the new hose to the vehicle.
2. Remove the cap from the washer pump outlet and install the new hose to the outlet of the pump.
3. Position the hose (1) to the air inlet panel (4).
4. Secure the hose to the air inlet grille panel.
5. Connect the hose to the washer nozzles. Refer to Washer Nozzle Replacement .
6. Install the air inlet grille panel. Refer to Air Inlet Grille Panel Replacement.
7. Top off the washer solvent container with washer solvent.
8. Close the hood.