For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the insulator clamp bolts.
3. Remove the clamps.
4. Remove the insulators.
5. Inspect all of the parts for wear and damage.

### Installation Procedure

1. Install the insulators to the stabilizer shaft .
2. Install the clamps over the insulators and the stabilizer shaft.

Notice: Refer to Fastener Notice in the Preface section.

3. Install insulator clamp bolts.

Tighten
Tighten the bolts to 50 N·m (37 lb ft).

4. Lower the vehicle.