For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Release the retainer on the daytime running lights (DRL), park lamp assembly.
3. Remove the DRL, park lamp assembly.
4. Use a flat-bladed tool in order to release the retainers that retain the grille to the body.
5. Lift the grille out of position.
6. Remove the grille from the vehicle.
7. Remove the nuts retaining the grille bar (1) to the grille (2).
8. Remove the grille bar.

### Installation Procedure

1. Position the grille to the grille molding.
2. Using a Weller® model 8200 soldering gun, or equivalent, equipped with a flat tip, use a circular motion around the heat stake.

2.1. | Apply firm steady pressure to spread the heat stake material onto the grille panel to achieve a proper weld.

2.2. | Heat stake the grille to the grille molding at all heat stake locations.

3. Install the grille bar (1).

Caution: Refer to Fastener Caution in the Preface section.

4. Install the grille bar retaining nuts and tighten to 4 N·m (35 lb in).
5. Position the grille to the vehicle.
6. Position the grille onto the radiator support such that the lower locating tabs are properly aligned.
7. Push the lower portion of the grille rearward until an audible engagement of the retainers is heard.
8. Align the upper locating tabs of the grille with the slots in the radiator support.
9. Install and fully seat the retaining clips into the radiator support.
10. Install the DRL, park lamp assembly.
11. Lower the hood.