For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accelerator Pedal Position (APP) Sensor Mounting Nut | 9 N·m | 80 lb in
Air Cleaner Assembly Bolt | 10 N·m | 89 lb in
Air Cleaner Assembly Nut | 15 N·m | 11 lb ft
Air Cleaner Outlet Duct Clamp | 6 N·m | 53 lb in
Air Cleaner Resonator Bolt | 6 N·m | 53 lb in
Air Cleaner Resonator Outlet Duct Clamp | 6 N·m | 53 lb in
Camshaft Position (CMP) Actuator Solenoid Valve Bolt | 10 N·m | 89 lb in
Camshaft Position (CMP) Sensor Bolt | 10 N·m | 89 lb in
Crankshaft Position (CKP) Sensor Bolt | 10 N·m | 89 lb in
Engine Coolant Temperature (ECT) Sensor | 14 N·m | 124 lb in
Evaporative Emission (EVAP) Canister Bolt | 25 N·m | 18 lb ft
Evaporative Emission (EVAP) Canister Purge Solenoid Valve Bolt | 10 N·m | 89 lb in
Fuel Filler Hose Clamp | 2.5 N·m | 22 lb in
Fuel Filler Hose Ground Strap Bolt | 9 N·m | 80 lb in
Fuel Filler Hose Screw | 2 N·m | 18 lb in
Fuel Pressure Regulator Screw | 8 N·m | 71 lb in
Fuel Rail Bolt | 10 N·m | 89 lb in
Fuel Tank Strap Bolt | 32 N·m | 24 lb ft
Heated Oxygen Sensor (HO2S) | 42 N·m | 31 lb ft
Ignition Coil Bolt | 10 N·m | 89 lb in
Knock Sensor (KS) Bolt | 25 N·m | 18 lb ft
Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor Screw | 2.25 N·m | 20 lb in
Secondary Air Injection (AIR) Check Valve Stud | 25 N·m | 18 lb ft
Secondary Air Injection (AIR) Pump Nut | 9 N·m | 80 lb in
Spark Plug | 18 N·m | 13 lb ft
Throttle Control Module Bolt | 10 N·m | 89 lb in