For 1990-2009 cars

### Removal Procedure

1. Remove the endgate from the vehicle. Refer to Endgate Replacement .
2. Remove the bolts retaining the endgate hinge to the body.
3. Remove the endgate hinge from the body.

### Installation Procedure

1. Install the endgate hinge to the body.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts retaining the endgate hinge to the body.

Tighten
Tighten the endgate hinge bolts to 20 N·m (15 lb ft).

3. Install the endgate to the vehicle. Refer to Endgate Replacement .