For 1990-2009 cars

## Rear Seat Belt Buckle Replacement Crew Cab

### Removal Procedure

1. Remove the rear bench seat from the vehicle. Refer to Rear Bench Seat Replacement .
2. Remove the grommet securing the rear seat belt buckle assembly to the seat.
3. Remove the rear seat belt buckle assembly from the seat cushion.

### Installation Procedure

1. Install the rear bench seat in the vehicle. Refer to Rear Bench Seat Replacement . Do not install the rear bench seat mounting nut.
2. Install the rear seat belt buckle through the seat cushion loop and position the seat belt buckle assembly over the rear bench seat mounting hole.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the rear bench seat mounting nut.

Tighten
Tighten the rear bench seat mounting nut to 52.5 N·m (39 lb ft).

## Rear Seat Belt Buckle Replacement Extended Cab

### Removal Procedure

1. Remove the rear folding seat from the vehicle. Refer to Folding Seat Replacement .
2. Remove the rear seat belt buckle assembly (1) from the vehicle.

### Installation Procedure

1. Position the rear seat belt buckle assembly (1) in the vehicle under the inboard leg (2) of the rear folding seat.
2. Install the rear folding seat in the vehicle. Refer to Folding Seat Replacement .