For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Support the rear axle at ride height.

Note: Do not attempt to hold the stabilizer shaft link near the boot. Use the hex feature on the end of the stud. Failure to do so could damage the boot.

3. Remove the stabilizer shaft link upper nut.
4. Remove the stabilizer shaft link lower nut.
5. Remove the stabilizer shaft link.

### Installation Procedure

Note: Do not attempt to hold the stabilizer shaft link near the boot. Use the hex feature on the end of the stud. Failure to do so could damage the boot.

1. Install the stabilizer shaft link.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the stabilizer shaft link mounting nuts.

• | Tighten the stabilizer bar link lower mounting nut to 44 N·m (32 lb ft).

• | Tighten the stabilizer bar link upper mounting nut to 44 N·m (32 lb ft).

3. Remove the axle support.
4. Lower the vehicle.