For 1990-2009 cars

### Removal Procedure

Notice: Refer to Differential Housing Cover and Gasket Removal Notice in the Preface section.

Important: The gasket and rear cover are reusable. Replace them only if they are damaged.

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the bolt for the rear brake pipe retainer.
3. Remove the bolt for the mounting bracket.
4. Remove the mounting brackets from the rear axle cover.
5. Position a suitable drain pan under the axle.
6. Remove the rear cover mounting bolts.
7. Remove the rear cover and gasket from the differential housing.
8. Drain the rear axle.

### Installation Procedure

1. Clean the contact area for the rear cover and gasket and the differential housing.
2. Install the retainer and mounting bracket for the rear brake pipe.
3. Install the mounting bolt for the mounting bracket.
4. Finger tighten the bolt for the mounting bracket.
5. Install the axle housing cover and gasket.

Notice: Refer to Fastener Notice in the Preface section.

6. Install the mounting bolts.

Tighten
Tighten the mounting bolts to 30 N·m (22 lb ft).

7. Install the retaining bolt for the brake pipe retainer.

Tighten
Tighten the mounting bolts to 20 N·m (14 lb ft).

8. Fill the rear axle with fluid. Refer to Rear Axle Lubricant Level Inspection .
9. Lower the vehicle.