For 1990-2009 cars

#### Tools Required

J 43631 Ball Joint Separator

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the rear brake drum. Refer to Brake Drum Replacement .
3. Using the J 43631 , remove the wheel stud.

### Installation Procedure

1. Position the wheel stud in the axle flange .
2. Install the 4 washers and the lug nut to the stud.
3. Tighten the lug nut until the stud fully seats.
4. Remove the lug nut and the washers.
5. Install the rear brake drum. Refer to Brake Drum Replacement .
6. Lower the vehicle.