For 1990-2009 cars

#### Tools Required

• | J 8092 Universal Driver Handle- ¾ in - 10

• | J 21128 Axle Pinion Oil Seal Installer

• | J 23690 Bearing Installer

• | J 2619-01 Slide Hammer

• | J 44685 Rear Axle Seal and Bearing Remover

### Removal Procedure

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation .
3. Remove the axle shaft. Refer to Rear Axle Shaft Replacement .
4. Using the J 44685 and the J 2619-01 , remove the axle shaft bearing and seal.

### Installation Procedure

1. Using the J 23690 and the J 8092 , install the axle bearing.
2. Using the J 21128 , install the axle shaft seal.
3. Install the axle shaft. Refer to Rear Axle Shaft Replacement .
4. Install the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation .
5. Fill the rear axle with axle lubricant. Use the proper fluid. Refer to Rear Axle Lubricant Replacement .
6. Lower the vehicle.