For 1990-2009 cars

### Removal Procedure

1. Remove the air inlet grille. Refer to Grille Replacement .
2. Disconnect the electrical connector to the ambient air temperature sensor.
3. Release the tabs (1) retaining the sensor to the radiator support bracket.
4. Remove the sensor (1) from the radiator support bracket.

### Installation Procedure

1. Position the sensor (1) to the radiator support bracket.
2. Install the sensor ensuring the retaining tabs (1) are fully seated to the radiator support bracket.
3. Connect the electrical connector to the ambient air temperature sensor.
4. Install the air inlet grille. Refer to Grille Replacement .