For 1990-2009 cars

Crew cab shown, others similar.

### Removal Procedure

1. Open the front and rear door, as necessary.
2. Remove the auxiliary weatherstrip by pulling the weatherstrip (1) from the roof pinchweld flange (2).

### Installation Procedure

1. Install the auxiliary weatherstrip to the roof pinchweld flange by pressing the weatherstrip (1) onto the roof flange (2), until it is fully seated.
2. Close the front and rear door, as necessary.