For 1990-2009 cars

### General Method

1. Verify that the leak is transmission fluid.
2. Thoroughly clean the suspected leak area.
3. Operate the vehicle for 24 km (15 mi), or until normal operating temperatures are reached.
4. Park the vehicle over clean paper or cardboard.
5. Shut OFF the engine.
6. Look for fluid spots on the paper.
7. Make the necessary repairs.

### Powder Method

1. Thoroughly clean the suspected leak area with solvent.
2. Apply an aerosol type powder, such as foot powder, to the suspected leak area.
3. Operate the vehicle for 24 km (15 mi), or until normal operating temperatures are reached.
4. Shut OFF the engine.
5. Inspect the suspected leak area.
6. Trace the leak path through the powder in order to find the source of the leak.
7. Make the necessary repairs.

### Dye and Black Light Method

A fluid dye and black light kit is available from various tool manufacturers.

1. Follow the manufacturer's instructions in order to determine the amount of dye to use.
2. Detect the leak with the black light.
3. Make the necessary repairs.

### Find the Cause of the Leak

Pinpoint the leak and trace the leak back to the source. You must determine the cause of the leak in order to repair the leak properly. For example, if you replace a gasket, but the sealing flange is bent, the new gasket will not repair the leak. You must also repair the bent flange. Before you attempt to repair a leak, check for the following conditions, and make repairs as necessary:

#### Gaskets

• | Fluid level/pressure is too high

• | Plugged vent or drain-back holes

• | Improperly tightened fasteners

• | Dirty or damaged threads

• | Warped flanges or sealing surface

• | Scratches, burrs, or other damage to the sealing surface

• | Damaged or worn gasket

• | Cracking or porosity of the component

• | Improper sealant used, where applicable

• | Incorrect gasket

#### Seals

• | Fluid level/pressure is too high

• | Plugged vent or drain-back holes

• | Damaged seal bore

• | Damaged or worn seal

• | Improper installation

• | Cracks in component

• | Manual or output shaft surface is scratched, nicked, or damaged

• | Loose or worn bearing causing excess seal wear

• | Damaged ISS O-Ring

### Possible Points of Fluid Leaks

#### Transmission Oil Pan

• | Incorrectly tightened oil pan bolts

• | Improperly installed or damaged oil pan gasket

• | Damaged oil pan or mounting face

• | Incorrect oil pan gasket

#### Case Leak

• | Damaged or missing fill tube seal

• | Mislocated fill tube bracket

• | Damaged vehicle speed sensor seal

• | Damaged manual shaft seal

• | Loose or damaged oil cooler connector fittings

• | Worn or damaged propeller shaft oil seal

• | Loose line pressure pipe plug

• | Warped

• | Distorted torque converter housing

• | Porous casting

#### Leak at the Torque Converter End

• | Converter leak in the weld area

• | Converter seal lip cut. Check the converter hub for damage

• | Converter seal bushing moved forward and damaged

• | Converter seal garter spring missing from the seal

• | Porous casting of the transmission case or the oil pump

#### Leak at the Vent Pipe or the Fluid Fill Tube

• | Overfilled system

• | Water or coolant in the fluid--the fluid will appear milky.

• | Transmission case porous

• | Incorrect fluid level indicator

• | Plugged vent

• | Drain-back holes plugged

• | Mispositioned oil pump to case gasket, if equipped

• | ISS or ISS plug loose

• | ISS O-Ring cut or damaged

#### Leak Inspection Points

(1) | Wiring Harness Pass-Through Connector O-ring Seal
(2) | Transmission Vent Assembly
(3) | Converter Housing to Case Joint (Pump to Case Oil Seal)
(4) | Line Pressure Plug
(5) | Case Extension to Case Seal
(6) | Manual Shaft Seal
(7) | Case Extension Oil Seal Assembly
(8) | Torque Converter Assembly
(9) | Pump to Case Oil Seal
(10) | Pump Oil Seal Assembly
(11) | Internal Transmission Speed Sensor to Case O-ring Seal - Some Models
(12) | 2-4 Servo Cover O-ring Seal
(13) | Oil Fill Tube Seal
(14) | Oil Cooler Pipe Connectors
(15) | Transmission Case
(16) | Transmission Oil Pan Gasket