For 1990-2009 cars

### Removal Procedure

1. Open the rear side access door.
2. Remove the wedge from the side access door by squeezing the retainer clip on the wedge and rotating the wedge downward.

### Installation Procedure

1. Install the wedge to the side access door by inserting the tabs into the slots on the door and rotating the wedge up until the retaining clip is fully seated.
2. Close the rear side access door.