For 1990-2009 cars

### Removal Procedure

1. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation

Important: DO NOT reuse the wheel drive shaft nut, replace with new.

2. Remove the wheel drive shaft nut and washer.
3. Remove the steering knuckle assembly. Refer to Steering Knuckle Replacement .
4. Release the wheel drive shaft by placing a brass drift against the tripod housing. Firmly strike the brass drift with a hammer to release the drive shaft. Left side shown, right side similar.
5. Remove the front wheel drive shaft from the vehicle.

### Installation Procedure

Important: When installing the front wheel drive shaft, a snap or pop should be heard and felt when the front wheel drive shaft is properly seated in the differential case.

1. Install the front wheel drive shaft in the front differential.
2. Install the steering knuckle assembly. Refer to Steering Knuckle Replacement .

Notice: Refer to Fastener Notice in the Preface section.

3. Install the new front wheel drive shaft nut and washer.

Tighten
Tighten the front wheel drive shaft nut to 260 N·m (191 lb ft).

4. Check the fluid level of the front differential. Add fluid if necessary. Refer to Front Axle Lubricant Replacement .
5. Install the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation .
6. Lower the vehicle.