For 1990-2009 cars

#### Tools Required

J 38778 Door Trim Pad Clip Remover or Equivalent

### Removal Procedure

1. Open the front and rear side access doors.
2. Remove the upper molded detail from the front of the side access door, by inserting J 38778 under the weatherstrip mold and releasing the integral retaining pins (3) on the mold to the door.
3. Remove the lower molded detail from the front of the side access door, by inserting J 38778 under the weatherstrip mold and releasing the integral retaining pins (1) on the mold to the door.
4. Remove the weatherstrip from around the door, by inserting J 38778 under the weatherstrip on releasing the integral pins from the door.
5. Remove the weatherstrip from the side access door.

### Installation Procedure

1. Position the weatherstrip to the rear side access door.
2. Install the upper molded detail to the front of the rear side access door using the integral retaining pins (1).
3. Install the lower molded detail to the front of the rear side access door using the integral retaining pins (1).
4. Install the weatherstrip around the rear door frame using the integral retainers.
5. Close the front and rear side access doors.