ENGINE STALL/HESITATION AFTER COLD START AND DRIVEAWAY. Oldsmobile Firenza 1986

For 1990-2009 cars

# ENGINE STALL/HESITATION AFTER COLD START AND DRIVEAWAY

#### MODELS/YEARS: 1986 FIRENZA MODELS WITH 2.8L MPFI ENGINE AND 3-SPEED TRANSAXLE

Some 1986 Firenzas with 2.8L MPFI engines (VIN Code W) and 3-speed automatic transaxles may experience a cold start stall or a hesitation during a cold driveaway.

To repair this condition, replace the PROM with one of the following service PROMs obtained from GMSPO.

Emission Air Old Service New Service PROM System Conditioning PROM Part Number Part Number ------ ------------ ---------------- -----------

Federal Yes 1228118 16126446 Federal No 1228119 16126447 Calif. Yes 1228120 16126448 Calif. No 1228121 16126450

#### NOTICE: The above service PROMs are for Firenzas with a 2.8L Port Fuel Injected engine, and an automatic 3-speed transaxle.

Use applicable labor time and operation numbers.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.