DTC P0602 Control Module Not Programmed. Oldsmobile Shelby Series 1 1999

For 1990-2009 cars

### Circuit Description

This diagnostic trouble code (DTC) indicates that the powertrain control module (PCM) internal electrically erasable programmable read only memory (EEPROM) is not flashed with any vehicle software. If you install a service PCM and do not flash the EEPROM, the engine will not run. This DTC indicates that an unflashed PCM causes the engine cranks but will not run situation.

### Conditions for Running the DTC

The ignition switch is in the run position.

### Conditions for Setting the DTC

No software data is present in the PCM.

### Action Taken When the DTC Sets

• | The PCM illuminates the malfunction indicator lamp (MIL) when the diagnostic runs and fails.

• | The PCM records the operating conditions at the time the diagnostic fails. The PCM stores this information in the Freeze Frame and/or Failure Records.

### Conditions for Clearing the MIL/DTC

• | The PCM turns OFF the malfunction indicator lamp (MIL) after 3 consecutive ignition cycles that the diagnostic runs and does not fail.

• | A last test failed, or current DTC, clears when the diagnostic runs and does not fail.

• | A history DTC clears after 40 consecutive warm-up cycles, if no failures are reported by this or any other emission related diagnostic.

• | Use a scan tool in order to clear the MIL and the DTC.

### Test Description

The number below refers to the step number on the diagnostic table.

1. If the flashing routine fails, verify that the equipment used is functioning properly and that all cable connections are clean and tight. Also, make sure that the software you download is correct for the PCM being flashed. If everything is OK, and a second attempt fails, the PCM is faulty.

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Powertrain On-Board Diagnostic (OBD) System Check? | -- | Go to Step 2 | Go to Powertrain On Board Diagnostic (OBD) System Check
2 | Flash the PCM with the correct software. Refer to Powertrain Control Module Replacement/Programming . Does DTC P0602 reset? | -- | Go to Step 3 | Go to Step 5

3

1. Verify that the equipment being used is functioning properly and that all the cable connections are clean and tight.
2. Attempt to flash the PCM again.

Does DTC P0602 reset?

--

Go to Step 4

Go to Step 5

4 | Important:: The replacement PCM must be programmed. Replace the PCM. Refer to Powertrain Control Module Replacement/Programming . Is the action complete? | -- | Go to Step 5 | --

5

1. Select the Diagnostic Trouble Code (DTC) option and the Clear DTC Information option using the scan tool.
2. Idle the engine at the normal operating temperature.
3. Select the Diagnostic Trouble Code (DTC) option and the Specific DTC option, then enter the DTC number using the scan tool.
4. Operate the vehicle within the Conditions for Running the DTC as specified in the supporting text, if applicable.

Does the scan tool indicate that this test ran and passed?

--

Go to Step 6

Go to Step 2

6 | Select the Capture Info option and the Review Info option using the scan tool. Does the scan tool display any DTCs that you have not diagnosed? | -- | Go to the applicable DTC table | System OK