Evaporative Emission Canister Purge Solenoid Replacement. Oldsmobile Shelby Series 1 1999

For 1990-2009 cars

### Removal Procedure

1. Remove the engine dress cover (2).
2. Remove the solenoid quick-connect hose (3) at the evaporative emission (EVAP) canister purge solenoid (4).
3. Remove the solenoid quick-connect hose (7) from the EVAP canister purge solenoid (4) to the enhanced EVAP service port (8).
4. Remove the electrical connector (6) at the EVAP canister purge solenoid.
5. Remove the EVAP canister purge (2) solenoid valve bolt.
6. Remove the EVAP canister purge solenoid tab from the bracket (5).

### Installation Procedure

1. Install the EVAP canister purge solenoid valve (4) to the bracket (5).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the EVAP canister purge 2) solenoid valve bolt.

Tighten
Tighten the bolt to 10 N·m (88 lb in).

3. Install the solenoid quick-connect hose (3) at the EVAP canister purge solenoid.
4. Install the solenoid quick-connect hose (7) from the EVAP canister purge solenoid to the enhanced EVAP service port.
5. Install the electrical connector (6) to the EVAP canister purge solenoid.
6. Install the engine dress cover (2).