Heated Oxygen Sensor Replacement - Bank 1 Sensor 1. Oldsmobile Shelby Series 1 1999

For 1990-2009 cars

### Removal Procedure

Notice: Remove oxygen sensors with the engine temperature above 48°C (120°F). Otherwise the oxygen sensors may be difficult to remove.

Notice: Take care when handling oxygen sensors. The electrical connector and louvered end must be kept free of contaminants. Do not use cleaning solvents on the sensor. Do not drop or mishandle the sensor.

Notice: A special anti-seize compound is used on the oxygen sensor threads. New service sensors should already have the compound applied to the threads. Coat the threads of a reused sensor with anti-seize compound P/N 5613695 or equivalent.

Caution: To avoid any vehicle damage, serious personal injury or death when major components are removed from the vehicle and the vehicle is supported by a hoist, support the vehicle with jack stands at the opposite end from which the components are being removed and strap the vehicle to the hoist.

1. Raise and support the vehicle.
2. Disconnect the right front oxygen sensor connector.
3. Remove the right front oxygen sensor from the exhaust pipe.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the right front oxygen sensor in the exhaust pipe.

Tighten
Tighten the right front HO2S sensor to 41 N·m (30 lb ft).

2. Connect the right front oxygen sensor connector.
3. Lower the vehicle.