LOW OIL LEVEL MESSAGE NORMAL OPERATION. Oldsmobile Toronado 1989

For 1990-2009 cars

# LOW OIL LEVEL MESSAGE NORMAL OPERATION

#### SUBJECT: LOW OIL LEVEL MESSAGE NORMAL OPERATION

#### MODELS/YEARS: 1988-91 TORONADO AND TROFEO

This bulletin supplements Dealer Technical Bulletin 90-T-179.

Some 1988-1991 Toronado and Trofeo Models that have been parked at an angle (i.e., on a hill or two wheels in a ditch) either front to back or side to side may exhibit a false low oil message. The angle of the vehicle causes the oil in the oil pan to flow away from the oil level switch. This condition is normal and will not be corrected by replacing the oil level switch or oil pan.

If the low oil message occurs on level surfaces, (88-90 model vehicles) refer to Dealer Technical Bulletin 90- T-179 for diagnosis. Use the 1991 Toronado/Trofeo Service Manual 8D2-88 to diagnose this condition on 1991 models.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.