OIL DRIPS OFF AXLE OR CRADLE AFTER OIL FILTER CHANGE. Oldsmobile Toronado 1991

For 1990-2009 cars

# OIL DRIPS OFF AXLE OR CRADLE AFTER OIL FILTER CHANGE

#### SUBJECT: OIL DRIPS OFF AXLE OR FRAME WHEN OIL FILTER IS REMOVED NEW OIL DRIP PAN ASSEMBLY

#### MODELS/YEARS: 1991 NINETY-EIGHT AND TORONADO

CONDITION: Some owners of the above vehicles may comment that oil drips off the frame or axle onto the garage floor shortly after an oil filter change.

CORRECTION: An oil drip pan assembly (P/N 24500643) and fastener (P/N 24501057) have been released for service. Parts are available from GMSPO.

#### Installation Procedure:

1. Raise the vehicle. 2. Snap drip pan onto studs as shown in the illustration. 3. Press fastener P/N 24501057 into the transaxle extension housing to secure drain end of the drip pan. 4. Lower vehicle.

#### WARRANTY INFORMATION:

Labor Operation Number: J0962 Labor Time: 0.2 hour Trouble Code: 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.